1. **获取def表中定义的子系统**

|  |  |
| --- | --- |
| url | http://127.0.0.1:60012/WebService/GetSubsystemDef |
| 请求方式 | get |
| 参数: | 无 |
| 返回值 | [ {  "SubsysCode" : 100000000,  "SubsysDesc" : "对新风机组，空调机组，空调冷热源，送排风系统的运行参数进行监测和记录；根据需求对各可控的运行参数进行控制；针对异常状况发出告警并记录告警信息；设置自动运行模式，达到智能、节能的目的。",  "SubsysName" : "暖通空调"  }, {  "SubsysCode" : 110000000,  "SubsysDesc" : "对于照明设备进行监视与控制。设备照明设备的运行模式，在满足人性化需求的情况下，达到绿色节能的目的。",  "SubsysName" : "照明系统"  }, {  "SubsysCode" : 120000000,  "SubsysDesc" : "对高压进出线运行参数，低压配电运行参数，备用电压运行参数，变配电机房运行参数的相关数据进行实时监测和记录；针对异常参数发出告警并记录告警信息；设置自动运行模式，达到智能、节能的目的。",  "SubsysName" : "变配电"  }, {  "SubsysCode" : 130000000,  "SubsysDesc" : "对生活水系统，污水排放系统，冷却水，雨水回收系统，消防水系统的各项数据进行实时监测和记录；针对异常参数发出告警并记录告警信息；设置自动运行模式，达到智能、节能的目的。",  "SubsysName" : "给排水"  }, {  "SubsysCode" : 140000000,  "SubsysDesc" : "电梯子系统集中监管所有直梯和扶梯的报警信息，集中显示设备的运行状态，可通关过集成平台远程监视各电梯设备现场情况。",  "SubsysName" : "电梯运行"  }, {  "SubsysCode" : 150000000,  "SubsysDesc" : "对于电、水、气能源消耗进行分类监视与统计。",  "SubsysName" : "能耗统计"  }, {  "SubsysCode" : 160000000,  "SubsysDesc" : "防盗子系统采用物理方法和电子技术，自动探测发生在布防监测区域内的侵入行为，产生报警信号，并显示报警位置、处理建议等信息。",  "SubsysName" : "周界防盗"  }, {  "SubsysCode" : 170000000,  "SubsysDesc" : "主要用于监控巡更设备信息，巡更路线及巡更时间，记录分析巡更任务执行情况",  "SubsysName" : "电子巡更"  }, {  "SubsysCode" : 180000000,  "SubsysDesc" : "门禁系统又称为出入管理控制系统，它集微机自动识别技术和现代安全管理措施为一体，由控制器、读卡器、电控锁、开门按钮组成，通过网络和门禁软件来管理系统中所有的信息分析和处理。门禁子系统是利用门禁系统中的门禁管理软件来对门禁系统进行管理，属于智能楼宇综合管理平台的一个子系统。",  "SubsysName" : "门禁管理"  }, {  "SubsysCode" : 190000000,  "SubsysDesc" : "利用视频技术探测、监视设防区域并实时显示、记录现场图像的电子系统或网络",  "SubsysName" : "视频监控"  }, {  "SubsysCode" : 200000000,  "SubsysDesc" : "IP网络广播系统是一套基于IP数据网络传输的音频扩音系统，可以在同网段的局域网内，跨网关的局域网内或Internet网上使用。广播子系统是利用广播网络服务器对IP网络广播系统进行管理，属于智能楼宇综合管理平台的一个子系统。",  "SubsysName" : "广播"  }, {  "SubsysCode" : 210000000,  "SubsysDesc" : "主要用于信息发布子系统",  "SubsysName" : "信息发布"  }, {  "SubsysCode" : 220000000,  "SubsysDesc" : "通过在特定区域安装客流统计设备，精准的统计出实时客流进出人数的系统",  "SubsysName" : "客流统计"  }, {  "SubsysCode" : 230000000,  "SubsysDesc" : "主要用于监控停车场设备工作状态、车位泊车状态和车辆流量数据",  "SubsysName" : "停车管理"  }, {  "SubsysCode" : 240000000,  "SubsysDesc" : "消防子系统实现消防设备监测功能。包括：实现漏电火灾报警、感温电缆、气体灭火控制系统、水炮控制系统、燃气报警系统、火灾自动报警系统的融合，在电子地图上显示各报警故障点位的位置。",  "SubsysName" : "消防系统"  }, {  "SubsysCode" : 250000000,  "SubsysDesc" : "主要用于楼宇对讲子系统",  "SubsysName" : "楼宇对讲"  }, {  "SubsysCode" : 260000000,  "SubsysDesc" : "智慧路灯",  "SubsysName" : "智慧路灯"  }, {  "SubsysCode" : 270000000,  "SubsysDesc" : "充电桩",  "SubsysName" : "充电桩"  }, {  "SubsysCode" : 280000000,  "SubsysDesc" : "一键报警",  "SubsysName" : "一键报警"  }, {  "SubsysCode" : 290000000,  "SubsysDesc" : "WIFI登录",  "SubsysName" : "WIFI"  } ] |

**2、获取def表中定义的模块**

|  |  |
| --- | --- |
| url | <http://127.0.0.1:60012/WebService/GetModuleDef> |
| 请求方式 | get |
| 参数: | 无 |
| 返回值 | [ {  "HasPattern" : false,  "ModCode" : 100100000,  "ModDesc" : "主要用于空调的冷源供应，对于冷源设备的监视与控制",  "ModName" : "冷冻模块",  "SubsysCode" : 100000000  }, {  "HasPattern" : false,  "ModCode" : 100200000,  "ModDesc" : "主要用于空调热源供应，对于供热的锅炉或市政供热管网进行监视与控制",  "ModName" : "供热模块",  "SubsysCode" : 100000000  }, {  "HasPattern" : false,  "ModCode" : 100300000,  "ModDesc" : "属于暖通空调子系统，负责监控空调机组的相关运行参数。",  "ModName" : "空调模块",  "SubsysCode" : 100000000  }, {  "HasPattern" : false,  "ModCode" : 100400000,  "ModDesc" : "属于暖通空调子系统，负责监控新风机组的相关运行参数。",  "ModName" : "新风模块",  "SubsysCode" : 100000000  }, {  "HasPattern" : false,  "ModCode" : 100500000,  "ModDesc" : "属于暖通空调子系统，用于显示各区域的环境参数。",  "ModName" : "环境监测",  "SubsysCode" : 100000000  }, {  "HasPattern" : false,  "ModCode" : 110100000,  "ModDesc" : "照明模块主要是办公照明、应急照明、窒外照明等照明模块的监视与控制",  "ModName" : "照明模块",  "SubsysCode" : 110000000  }, {  "HasPattern" : false,  "ModCode" : 120100000,  "ModDesc" : "属于变配电子系统，负责监控变配电系统的相关运行参数。",  "ModName" : "变配电模块",  "SubsysCode" : 120000000  }, {  "HasPattern" : false,  "ModCode" : 130100000,  "ModDesc" : "属于给排水子系统，负责监控给排水系统的相关运行参数。",  "ModName" : "给排水模块",  "SubsysCode" : 130000000  }, {  "HasPattern" : false,  "ModCode" : 140100000,  "ModDesc" : "电梯监控模块是电梯子系统的子集，目前电梯子系统只有一个电梯监控模块。",  "ModName" : "电梯监控",  "SubsysCode" : 140000000  }, {  "HasPattern" : false,  "ModCode" : 150100000,  "ModDesc" : "分区、分时、分场景电能耗的监测与统计",  "ModName" : "电能耗模块",  "SubsysCode" : 150000000  }, {  "HasPattern" : false,  "ModCode" : 150200000,  "ModDesc" : "分区、分时、分场景水能耗的监测与统计",  "ModName" : "水能耗模块",  "SubsysCode" : 150000000  }, {  "HasPattern" : false,  "ModCode" : 150300000,  "ModDesc" : "分区、分时、分场景气能耗的监测与统计",  "ModName" : "气能耗模块",  "SubsysCode" : 150000000  }, {  "HasPattern" : false,  "ModCode" : 160100000,  "ModDesc" : "周界入侵模块是周界防盗子系统的子集，目前周界防盗子系统只有一个周界入侵模块，以后可能会增加其他模块。",  "ModName" : "周界防盗",  "SubsysCode" : 160000000  }, {  "HasPattern" : false,  "ModCode" : 170100000,  "ModDesc" : "主要用于监控巡更设备信息，巡更路线及巡更时间，记录分析巡更任务执行情况",  "ModName" : "巡更模块",  "SubsysCode" : 170000000  }, {  "HasPattern" : false,  "ModCode" : 180100000,  "ModDesc" : "门禁子系统模块，连接门禁系统的管理软件或设备，通过厂商提供的接口对门禁系统进行管理",  "ModName" : "门禁",  "SubsysCode" : 180000000  }, {  "HasPattern" : false,  "ModCode" : 190100000,  "ModDesc" : "视频监控模块负责对需要进行监控的室内外场所进行有效的视频探测与监视，图像显示、记录与回放",  "ModName" : "视频",  "SubsysCode" : 190000000  }, {  "HasPattern" : false,  "ModCode" : 200100000,  "ModDesc" : "广播子系统模块，连接广播系统的管理软件或设备，通过厂商提供的接口对广播系统进行管理",  "ModName" : "广播",  "SubsysCode" : 200000000  }, {  "HasPattern" : false,  "ModCode" : 210100000,  "ModDesc" : "信息发布模块",  "ModName" : "信息发布",  "SubsysCode" : 210000000  }, {  "HasPattern" : false,  "ModCode" : 220100000,  "ModDesc" : "通过各种算法技术实时获取指定时段和指定区域内的客流数据，并对客流数据进行分析处理，显示客流的分布状态和变化趋势",  "ModName" : "客流统计",  "SubsysCode" : 220000000  }, {  "HasPattern" : false,  "ModCode" : 230100000,  "ModDesc" : "主要用于监控停车场设备工作状态、车位泊车状态和车辆流量数据",  "ModName" : "停车场管理模块",  "SubsysCode" : 230000000  }, {  "HasPattern" : false,  "ModCode" : 230200000,  "ModDesc" : "主要用于监控停车场的设备信息、车辆信息、过车记录等信息，但是不包括车位管理（特指车位状态和所停车辆信息可监控的车位管理）",  "ModName" : "停车场管理（无车位管理）",  "SubsysCode" : 230000000  }, {  "HasPattern" : false,  "ModCode" : 230300000,  "ModDesc" : "用于管理停车场的车位信息，只有车位状态（是否停车）、所停车辆信息可监测时，才会用到该模块，如果只有车位名称和编号可得知时，不认为是车位管理模块",  "ModName" : "车位管理模块",  "SubsysCode" : 230000000  }, {  "HasPattern" : false,  "ModCode" : 240100000,  "ModDesc" : "消防火灾模块是消防子系统的子集，目前消防子系统只有一个消防火灾模块。",  "ModName" : "消防火灾",  "SubsysCode" : 240000000  }, {  "HasPattern" : false,  "ModCode" : 250100000,  "ModDesc" : "楼宇对讲模块",  "ModName" : "楼宇对讲",  "SubsysCode" : 250000000  }, {  "HasPattern" : false,  "ModCode" : 260100000,  "ModDesc" : "智慧路灯模块",  "ModName" : "智慧路灯",  "SubsysCode" : 260000000  }, {  "HasPattern" : false,  "ModCode" : 270100000,  "ModDesc" : "充电桩模块",  "ModName" : "充电桩",  "SubsysCode" : 270000000  }, {  "HasPattern" : false,  "ModCode" : 280100000,  "ModDesc" : "一键报警模块",  "ModName" : "一键报警",  "SubsysCode" : 280000000  }, {  "HasPattern" : false,  "ModCode" : 290100000,  "ModDesc" : "WIFI登录模块",  "ModName" : "WIFI",  "SubsysCode" : 290000000  } ] |

**3 获取def表中定义的设备**

* **请求URL：**
* http://127.0.0.1:60012/WebService/GetDeviceDef
* **参数格式：**
* **请求方式：get**
* **参数：**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
|  |  |  |  |

* json返回示例：

[ {

"DevCode" : 100101000,

"DevDesc" : "冷水机组又称为：冷冻机、制冷机组、冰水机组、冷却设备等",

"DevName" : "冷水机组",

"ModCode" : 100100000

}, {

"DevCode" : 100102000,

"DevDesc" : "冷冻水泵,冷冻泵的作用是将经制冷机降温的冷冻水通过输送管道送到中央空调的各出风口处的风机盘管组件中,对环境起降温作用",

"DevName" : "冷冻泵",

"ModCode" : 100100000

}, {

"DevCode" : 100103000,

"DevDesc" : "冷却水泵用来循环冷却水，冷却水泵将升温后的冷却水压入冷却塔，使之与大气进行热交换，降温后送回主机冷凝器继续热交换",

"DevName" : "冷却泵",

"ModCode" : 100100000

}, {

"DevCode" : 100104000,

"DevDesc" : "冷却塔(The cooling tower)是用水作为循环冷却剂，从一系统中吸收热量排放至大气中，以降低水温的装置",

"DevName" : "冷却塔",

"ModCode" : 100100000

}, {

"DevCode" : 100105000,

"DevDesc" : "",

"DevName" : "补水泵",

"ModCode" : 100100000

}, {

"DevCode" : 100106000,

"DevDesc" : "",

"DevName" : "补水箱",

"ModCode" : 100100000

}, {

"DevCode" : 100107000,

"DevDesc" : "",

"DevName" : "膨涨水箱",

"ModCode" : 100100000

}, {

"DevCode" : 100201000,

"DevDesc" : "",

"DevName" : "锅炉",

"ModCode" : 100200000

}, {

"DevCode" : 100202000,

"DevDesc" : "",

"DevName" : "锅炉热水循环泵",

"ModCode" : 100200000

}, {

"DevCode" : 100203000,

"DevDesc" : "",

"DevName" : "锅炉热源系统",

"ModCode" : 100200000

}, {

"DevCode" : 100204000,

"DevDesc" : "",

"DevName" : "板式换热器",

"ModCode" : 100200000

}, {

"DevCode" : 100205000,

"DevDesc" : "",

"DevName" : "换热站热水循环泵",

"ModCode" : 100200000

}, {

"DevCode" : 100206000,

"DevDesc" : "",

"DevName" : "换热站热源系统",

"ModCode" : 100200000

}, {

"DevCode" : 100207000,

"DevDesc" : "",

"DevName" : "供回水管网",

"ModCode" : 100200000

}, {

"DevCode" : 100301000,

"DevDesc" : "组合式空调机组",

"DevName" : "组合式空调机组",

"ModCode" : 100300000

}, {

"DevCode" : 100302000,

"DevDesc" : "吊装式空调机组",

"DevName" : "吊装式空调机组",

"ModCode" : 100300000

}, {

"DevCode" : 100303000,

"DevDesc" : "空调末端",

"DevName" : "风机盘管",

"ModCode" : 100300000

}, {

"DevCode" : 100401000,

"DevDesc" : "新风机组",

"DevName" : "新风机组",

"ModCode" : 100400000

}, {

"DevCode" : 100501000,

"DevDesc" : "环境监测温度湿度传感器",

"DevName" : "环境监测传感器",

"ModCode" : 100500000

}, {

"DevCode" : 110101000,

"DevDesc" : "照明回路设备",

"DevName" : "组合照明回路",

"ModCode" : 110100000

}, {

"DevCode" : 110102000,

"DevDesc" : "照明回路设备",

"DevName" : "基本照明回路",

"ModCode" : 110100000

}, {

"DevCode" : 110103000,

"DevDesc" : "调光照明回路设备",

"DevName" : "无极调光回路",

"ModCode" : 110100000

}, {

"DevCode" : 120101000,

"DevDesc" : "",

"DevName" : "高压进出线",

"ModCode" : 120100000

}, {

"DevCode" : 120102000,

"DevDesc" : "",

"DevName" : "直流屏",

"ModCode" : 120100000

}, {

"DevCode" : 120103000,

"DevDesc" : "",

"DevName" : "变压器",

"ModCode" : 120100000

}, {

"DevCode" : 120104000,

"DevDesc" : "",

"DevName" : "低压电进线",

"ModCode" : 120100000

}, {

"DevCode" : 120105000,

"DevDesc" : "",

"DevName" : "低压电出线",

"ModCode" : 120100000

}, {

"DevCode" : 120106000,

"DevDesc" : "",

"DevName" : "柴油发电机",

"ModCode" : 120100000

}, {

"DevCode" : 120107000,

"DevDesc" : "",

"DevName" : "UPS/EPS",

"ModCode" : 120100000

}, {

"DevCode" : 120108000,

"DevDesc" : "",

"DevName" : "配电室环境",

"ModCode" : 120100000

}, {

"DevCode" : 120109000,

"DevDesc" : "",

"DevName" : "功率补偿",

"ModCode" : 120100000

}, {

"DevCode" : 130101000,

"DevDesc" : "",

"DevName" : "生活水泵",

"ModCode" : 130100000

}, {

"DevCode" : 130102000,

"DevDesc" : "",

"DevName" : "不锈钢水箱",

"ModCode" : 130100000

}, {

"DevCode" : 130103000,

"DevDesc" : "",

"DevName" : "机房环境",

"ModCode" : 130100000

}, {

"DevCode" : 130104000,

"DevDesc" : "",

"DevName" : "污水坑泵",

"ModCode" : 130100000

}, {

"DevCode" : 130105000,

"DevDesc" : "",

"DevName" : "污水集水池",

"ModCode" : 130100000

}, {

"DevCode" : 130106000,

"DevDesc" : "",

"DevName" : "隔油池",

"ModCode" : 130100000

}, {

"DevCode" : 130107000,

"DevDesc" : "",

"DevName" : "冷却水补水泵",

"ModCode" : 130100000

}, {

"DevCode" : 130108000,

"DevDesc" : "",

"DevName" : "雨水提升泵",

"ModCode" : 130100000

}, {

"DevCode" : 130109000,

"DevDesc" : "",

"DevName" : "雨水回收池",

"ModCode" : 130100000

}, {

"DevCode" : 130110000,

"DevDesc" : "",

"DevName" : "消火栓水泵",

"ModCode" : 130100000

}, {

"DevCode" : 130111000,

"DevDesc" : "",

"DevName" : "喷淋水泵",

"ModCode" : 130100000

}, {

"DevCode" : 130112000,

"DevDesc" : "",

"DevName" : "消防水炮泵",

"ModCode" : 130100000

}, {

"DevCode" : 130113000,

"DevDesc" : "",

"DevName" : "防护冷却水泵",

"ModCode" : 130100000

}, {

"DevCode" : 140101000,

"DevDesc" : "",

"DevName" : "梯控直梯",

"ModCode" : 140100000

}, {

"DevCode" : 140102000,

"DevDesc" : "",

"DevName" : "梯控扶梯",

"ModCode" : 140100000

}, {

"DevCode" : 140103000,

"DevDesc" : "",

"DevName" : "梯控机房环境",

"ModCode" : 140100000

}, {

"DevCode" : 140104000,

"DevDesc" : "",

"DevName" : "梯控电梯底坑",

"ModCode" : 140100000

}, {

"DevCode" : 150101000,

"DevDesc" : "电量监测",

"DevName" : "电表",

"ModCode" : 150100000

}, {

"DevCode" : 150201000,

"DevDesc" : "水量监测",

"DevName" : "水表",

"ModCode" : 150200000

}, {

"DevCode" : 150301000,

"DevDesc" : "气量监测",

"DevName" : "天燃气表",

"ModCode" : 150300000

}, {

"DevCode" : 160101000,

"DevDesc" : "",

"DevName" : "周界防盗传感器",

"ModCode" : 160100000

}, {

"DevCode" : 170101000,

"DevDesc" : "部署在待巡更位置的巡更点",

"DevName" : "巡更点",

"ModCode" : 170100000

}, {

"DevCode" : 180101000,

"DevDesc" : "门禁系统智能管理设备，负载整个系统输入、输出信息的处理和存储、控制等",

"DevName" : "门禁控制器",

"ModCode" : 180100000

}, {

"DevCode" : 180102000,

"DevDesc" : "门禁系统信号输入设备，读取卡片中的数据",

"DevName" : "门禁读卡器",

"ModCode" : 180100000

}, {

"DevCode" : 180103000,

"DevDesc" : "检测门的安全状态",

"DevName" : "门禁电锁",

"ModCode" : 180100000

}, {

"DevCode" : 190101000,

"DevDesc" : "视频设备",

"DevName" : "监控摄像机",

"ModCode" : 190100000

}, {

"DevCode" : 190102000,

"DevDesc" : "",

"DevName" : "数字矩阵",

"ModCode" : 190100000

}, {

"DevCode" : 190103000,

"DevDesc" : "",

"DevName" : "大屏幕显示设备",

"ModCode" : 190100000

}, {

"DevCode" : 190104000,

"DevDesc" : "",

"DevName" : "硬盘录像机",

"ModCode" : 190100000

}, {

"DevCode" : 190105000,

"DevDesc" : "",

"DevName" : "磁盘阵列",

"ModCode" : 190100000

}, {

"DevCode" : 200101000,

"DevDesc" : "",

"DevName" : "广播终端设备",

"ModCode" : 200100000

}, {

"DevCode" : 210101000,

"DevDesc" : "",

"DevName" : "LED大屏幕",

"ModCode" : 210100000

}, {

"DevCode" : 210102000,

"DevDesc" : "",

"DevName" : "LED主机",

"ModCode" : 210100000

}, {

"DevCode" : 220101000,

"DevDesc" : "",

"DevName" : "客流视频设备",

"ModCode" : 220100000

}, {

"DevCode" : 230101000,

"DevDesc" : "停车场的道闸设备",

"DevName" : "道闸",

"ModCode" : 230100000

}, {

"DevCode" : 230102000,

"DevDesc" : "停车场的车位",

"DevName" : "车位",

"ModCode" : 230100000

}, {

"DevCode" : 230103000,

"DevDesc" : "停车场的车道，一个车道可能包括多个设备",

"DevName" : "车道",

"ModCode" : 230100000

}, {

"DevCode" : 240101000,

"DevDesc" : "",

"DevName" : "消防感温火灾探测器",

"ModCode" : 240100000

}, {

"DevCode" : 240102000,

"DevDesc" : "",

"DevName" : "消防感烟火灾探测器",

"ModCode" : 240100000

}, {

"DevCode" : 240103000,

"DevDesc" : "",

"DevName" : "消防感光火灾探测器",

"ModCode" : 240100000

}, {

"DevCode" : 240104000,

"DevDesc" : "",

"DevName" : "消防可燃气体探测器",

"ModCode" : 240100000

}, {

"DevCode" : 240105000,

"DevDesc" : "",

"DevName" : "消防复合火灾探测器",

"ModCode" : 240100000

}, {

"DevCode" : 240106000,

"DevDesc" : "",

"DevName" : "消防手动火灾报警按钮",

"ModCode" : 240100000

}, {

"DevCode" : 240107000,

"DevDesc" : "",

"DevName" : "消防火灾报警控制器",

"ModCode" : 240100000

}, {

"DevCode" : 240108000,

"DevDesc" : "",

"DevName" : "消防输入输出模块",

"ModCode" : 240100000

}, {

"DevCode" : 240109000,

"DevDesc" : "",

"DevName" : "消防水流指示器",

"ModCode" : 240100000

}, {

"DevCode" : 240110000,

"DevDesc" : "",

"DevName" : "消防阀门限位器",

"ModCode" : 240100000

}, {

"DevCode" : 240111000,

"DevDesc" : "",

"DevName" : "消防压力检测器",

"ModCode" : 240100000

}, {

"DevCode" : 240112000,

"DevDesc" : "",

"DevName" : "消防水力警铃",

"ModCode" : 240100000

}, {

"DevCode" : 240113000,

"DevDesc" : "",

"DevName" : "消防压力开关",

"ModCode" : 240100000

}, {

"DevCode" : 250101000,

"DevDesc" : "围墙机",

"DevName" : "围墙机",

"ModCode" : 250100000

}, {

"DevCode" : 250102000,

"DevDesc" : "门口主机",

"DevName" : "门口主机",

"ModCode" : 250100000

}, {

"DevCode" : 250103000,

"DevDesc" : "室内分机",

"DevName" : "室内分机",

"ModCode" : 250100000

}, {

"DevCode" : 250104000,

"DevDesc" : "管理机",

"DevName" : "管理机",

"ModCode" : 250100000

}, {

"DevCode" : 260101000,

"DevDesc" : "路灯灯杆",

"DevName" : "路灯灯杆",

"ModCode" : 260100000

}, {

"DevCode" : 270101000,

"DevDesc" : "充电桩",

"DevName" : "充电桩",

"ModCode" : 270100000

}, {

"DevCode" : 280101000,

"DevDesc" : "一键报警主机",

"DevName" : "一键报警主机",

"ModCode" : 280100000

}, {

"DevCode" : 290101000,

"DevDesc" : "WIFI接入点设备控制器",

"DevName" : "WIFI接入控制器",

"ModCode" : 290100000

}, {

"DevCode" : 290102000,

"DevDesc" : "WIFI接入点设备",

"DevName" : "WIFI接入点",

"ModCode" : 290100000

} ]

**4、获取def表中定义的属性配置详情列表**

* **请求URL：**
* http://127.0.0.1:60012/WebService/GetAttributeDef
* **参数格式：**
* **请求方式：get**
* **参数：**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
|  |  |  |  |

* json返回示例：

[ {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100001,

"AttrName" : "集水器压力",

"AttrType" : "监测",

"DisplayName" : "集水器压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100002,

"AttrName" : "旁通压差",

"AttrType" : "监测",

"DisplayName" : "旁通压差",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100003,

"AttrName" : "集水器进水温度",

"AttrType" : "监测",

"DisplayName" : "集水器进水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100100004,

"AttrName" : "分集水器压差设定值",

"AttrType" : "操作",

"DisplayName" : "分集水器压差设定值",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100005,

"AttrName" : "最不利末端压差1",

"AttrType" : "监测",

"DisplayName" : "最不利末端压差1",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100006,

"AttrName" : "最不利末端压差2",

"AttrType" : "监测",

"DisplayName" : "最不利末端压差1",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100007,

"AttrName" : "最不利末端压差3",

"AttrType" : "监测",

"DisplayName" : "最不利末端压差1",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100100008,

"AttrName" : "最不利末端压差设定值",

"AttrType" : "操作",

"DisplayName" : "最不利末端压差设定值",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 0,

"AttrCode" : 100100009,

"AttrName" : "冷冻水流量",

"AttrType" : "监测",

"DisplayName" : "冷冻水流量",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 1000.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "m3/h"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 0,

"AttrCode" : 100100010,

"AttrName" : "冷却水流量",

"AttrType" : "监测",

"DisplayName" : "冷却水流量",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 1000.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "m3/h"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100011,

"AttrName" : "冷冻水总供水温度",

"AttrType" : "监测",

"DisplayName" : "冷冻水总供水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100012,

"AttrName" : "冷冻水总回水温度",

"AttrType" : "监测",

"DisplayName" : "冷冻水总回水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100013,

"AttrName" : "冷却水总供水温度",

"AttrType" : "监测",

"DisplayName" : "冷却水总供水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100014,

"AttrName" : "冷却水总回水温度",

"AttrType" : "监测",

"DisplayName" : "冷却水总回水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100015,

"AttrName" : "冷冻水总供水压力",

"AttrType" : "监测",

"DisplayName" : "冷冻水总供水压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100016,

"AttrName" : "冷冻水总回水压力",

"AttrType" : "监测",

"DisplayName" : "冷冻水总回水压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100017,

"AttrName" : "冷却水总供水压力",

"AttrType" : "监测",

"DisplayName" : "冷却水总供水压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100018,

"AttrName" : "冷却水总回水压力",

"AttrType" : "监测",

"DisplayName" : "冷却水总回水压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 100.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100100019,

"AttrName" : "旁通阀位设定值",

"AttrType" : "操作",

"DisplayName" : "旁通阀位设定值",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : 100.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100100020,

"AttrName" : "旁通阀位",

"AttrType" : "监测",

"DisplayName" : "旁通阀位",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : 0.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100100021,

"AttrName" : "季节转换阀控制",

"AttrType" : "操作",

"DisplayName" : "季节转换阀控制",

"EnumVals" : "0:关闭;1:打开",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100100022,

"AttrName" : "季节转换阀开反馈",

"AttrType" : "状态",

"DisplayName" : "季节转换阀开反馈",

"EnumVals" : "0:未开启;1:开启",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100100023,

"AttrName" : "季节转换阀关反馈",

"AttrType" : "状态",

"DisplayName" : "季节转换阀关反馈",

"EnumVals" : "0:未关闭;1:关闭",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 40.00,

"AlarmLow" : -10.00,

"AlarmType" : 3,

"AttrCode" : 100100024,

"AttrName" : "冷水机房温度",

"AttrType" : "监测",

"DisplayName" : "冷水机房温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : -30.00,

"AlarmType" : 3,

"AttrCode" : 100100025,

"AttrName" : "室外温度",

"AttrType" : "监测",

"DisplayName" : "室外温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100100000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101001,

"AttrName" : "冷水机组开关控制",

"AttrType" : "操作",

"DisplayName" : "冷水机组开关控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101002,

"AttrName" : "冷水机组开关状态",

"AttrType" : "状态",

"DisplayName" : "冷水机组开关状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101003,

"AttrName" : "冷水机组故障",

"AttrType" : "告警",

"DisplayName" : "冷水机组故障",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101004,

"AttrName" : "冷水机组手自动",

"AttrType" : "状态",

"DisplayName" : "冷水机组手自动",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100101005,

"AttrName" : "冷冻水供水温度设定值",

"AttrType" : "操作",

"DisplayName" : "冷冻水供水温度设定值",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100101006,

"AttrName" : "冷冻水供水温度",

"AttrType" : "监测",

"DisplayName" : "冷冻水供水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100101007,

"AttrName" : "冷冻水回水温度",

"AttrType" : "监测",

"DisplayName" : "冷冻水回水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 40.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100101008,

"AttrName" : "冷却水出水温度",

"AttrType" : "监测",

"DisplayName" : "冷却水出水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 40.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100101009,

"AttrName" : "冷却水回水温度",

"AttrType" : "监测",

"DisplayName" : "冷却水回水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100101010,

"AttrName" : "冷冻水供水压力",

"AttrType" : "监测",

"DisplayName" : "冷冻水供水压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100101011,

"AttrName" : "冷冻水回水压力",

"AttrType" : "监测",

"DisplayName" : "冷冻水回水压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100101012,

"AttrName" : "冷却水出水压力",

"AttrType" : "监测",

"DisplayName" : "冷却水出水压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100101013,

"AttrName" : "冷却水回水压力",

"AttrType" : "监测",

"DisplayName" : "冷却水回水压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100101014,

"AttrName" : "冷凝温度",

"AttrType" : "监测",

"DisplayName" : "冷凝温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 20.00,

"AlarmLow" : -10.00,

"AlarmType" : 3,

"AttrCode" : 100101015,

"AttrName" : "蒸发温度",

"AttrType" : "监测",

"DisplayName" : "蒸发温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101016,

"AttrName" : "冷冻水流开关状态",

"AttrType" : "状态",

"DisplayName" : "冷冻水流开关状态",

"EnumVals" : "0:无水流;1:有水流",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101017,

"AttrName" : "冷却蝶阀控制启停",

"AttrType" : "操作",

"DisplayName" : "冷却蝶阀控制启停",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101018,

"AttrName" : "冷却蝶阀控制关反馈",

"AttrType" : "状态",

"DisplayName" : "冷却蝶阀控制关反馈",

"EnumVals" : "0:未停止;1:停止",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101019,

"AttrName" : "冷却蝶阀控制开反馈",

"AttrType" : "状态",

"DisplayName" : "冷却蝶阀控制开反馈",

"EnumVals" : "0:未启动;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101020,

"AttrName" : "冷冻蝶阀调节",

"AttrType" : "操作",

"DisplayName" : "冷冻蝶阀调节",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 2,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100101021,

"AttrName" : "冷冻蝶阀反馈",

"AttrType" : "状态",

"DisplayName" : "冷冻蝶阀反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 2,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100102001,

"AttrName" : "冷冻水泵启停控制",

"AttrType" : "操作",

"DisplayName" : "冷冻水泵启停控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100102002,

"AttrName" : "冷冻水泵启停状态",

"AttrType" : "状态",

"DisplayName" : "冷冻水泵启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100102003,

"AttrName" : "冷冻水泵故障报警",

"AttrType" : "告警",

"DisplayName" : "冷冻水泵故障报警",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100102004,

"AttrName" : "冷冻水泵手自动",

"AttrType" : "状态",

"DisplayName" : "冷冻水泵手自动",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100102005,

"AttrName" : "冷冻水泵变频调节",

"AttrType" : "操作",

"DisplayName" : "冷冻水泵变频调节",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100102000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100102006,

"AttrName" : "冷冻水泵变频状态",

"AttrType" : "状态",

"DisplayName" : "冷冻水泵变频状态",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100102000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100102007,

"AttrName" : "冷冻水泵水泵进口压力",

"AttrType" : "监测",

"DisplayName" : "冷冻水泵水泵进口压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100102000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100102008,

"AttrName" : "冷冻水泵水泵出口压力",

"AttrType" : "监测",

"DisplayName" : "冷冻水泵水泵出口压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100102000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100103001,

"AttrName" : "冷却水泵启停控制",

"AttrType" : "操作",

"DisplayName" : "冷却水泵启停控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100103002,

"AttrName" : "冷却水泵启停状态",

"AttrType" : "状态",

"DisplayName" : "冷却水泵启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100103003,

"AttrName" : "冷却水泵故障报警",

"AttrType" : "告警",

"DisplayName" : "冷却水泵故障报警",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100103004,

"AttrName" : "冷却水泵手自动",

"AttrType" : "状态",

"DisplayName" : "冷却水泵手自动",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100103005,

"AttrName" : "冷却水泵变频调节",

"AttrType" : "操作",

"DisplayName" : "冷却水泵变频调节",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100103000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100103006,

"AttrName" : "冷却水泵变频状态",

"AttrType" : "状态",

"DisplayName" : "冷却水泵变频状态",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100103000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100103007,

"AttrName" : "冷却水泵水泵进口压力",

"AttrType" : "监测",

"DisplayName" : "冷却水泵水泵进口压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100103000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100103008,

"AttrName" : "冷却水泵水泵出口压力",

"AttrType" : "监测",

"DisplayName" : "冷却水泵水泵出口压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100103000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100104001,

"AttrName" : "冷却塔启停控制",

"AttrType" : "操作",

"DisplayName" : "冷却塔启停控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100104002,

"AttrName" : "冷却塔启停状态",

"AttrType" : "状态",

"DisplayName" : "冷却塔启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100104003,

"AttrName" : "冷却塔故障报警",

"AttrType" : "告警",

"DisplayName" : "冷却塔故障报警",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100104004,

"AttrName" : "冷却塔手自动",

"AttrType" : "状态",

"DisplayName" : "冷却塔手自动",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100104005,

"AttrName" : "冷却塔变频调节",

"AttrType" : "操作",

"DisplayName" : "冷却塔变频调节",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 100104006,

"AttrName" : "冷却塔变频状态",

"AttrType" : "状态",

"DisplayName" : "冷却塔变频状态",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100104007,

"AttrName" : "冷却塔供水蝶阀状态",

"AttrType" : "状态",

"DisplayName" : "冷却塔供水蝶阀状态",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100104008,

"AttrName" : "冷却塔回水蝶阀状态",

"AttrType" : "状态",

"DisplayName" : "冷却塔回水蝶阀状态",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100104009,

"AttrName" : "冷却塔供水蝶阀控制",

"AttrType" : "操作",

"DisplayName" : "冷却塔供水蝶阀控制",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100104010,

"AttrName" : "冷却塔回水蝶阀控制",

"AttrType" : "操作",

"DisplayName" : "冷却塔回水蝶阀控制",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 50.00,

"AlarmLow" : 10.00,

"AlarmType" : 3,

"AttrCode" : 100104011,

"AttrName" : "冷却塔集水盘温度",

"AttrType" : "监测",

"DisplayName" : "冷却塔集水盘温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100104012,

"AttrName" : "冷却塔集水盘水液位",

"AttrType" : "监测",

"DisplayName" : "冷却塔集水盘水液位",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100104000,

"ValueMax" : 10000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mm"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100105001,

"AttrName" : "补水泵故障报警",

"AttrType" : "告警",

"DisplayName" : "补水泵故障报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100105000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100105002,

"AttrName" : "补水泵运行状态",

"AttrType" : "状态",

"DisplayName" : "补水泵运行状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100105000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100105003,

"AttrName" : "补水泵手自动模式",

"AttrType" : "状态",

"DisplayName" : "补水泵手自动模式",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100105000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100106001,

"AttrName" : "补水箱低水位报警",

"AttrType" : "告警",

"DisplayName" : "补水箱低水位报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100106000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100107001,

"AttrName" : "膨涨水箱超高水位报警",

"AttrType" : "告警",

"DisplayName" : "膨涨水箱超高水位报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100201001,

"AttrName" : "锅炉启停控制",

"AttrType" : "操作",

"DisplayName" : "锅炉启停控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100201000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100201002,

"AttrName" : "锅炉运行状态",

"AttrType" : "状态",

"DisplayName" : "锅炉运行状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100201000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100201003,

"AttrName" : "锅炉手自动模式",

"AttrType" : "状态",

"DisplayName" : "锅炉手自动模式",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100201000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100201004,

"AttrName" : "锅炉故障报警",

"AttrType" : "告警",

"DisplayName" : "锅炉故障报警",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100201000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100201005,

"AttrName" : "锅炉热水出水温度设定值",

"AttrType" : "操作",

"DisplayName" : "锅炉热水出水温度设定值",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100201000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100201006,

"AttrName" : "锅炉热水供水温度",

"AttrType" : "监测",

"DisplayName" : "锅炉热水供水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100201000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100201007,

"AttrName" : "锅炉热水回水温度",

"AttrType" : "监测",

"DisplayName" : "锅炉热水回水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100201000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100202001,

"AttrName" : "热水循环泵启停控制",

"AttrType" : "操作",

"DisplayName" : "热水循环泵启停控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100202000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100202002,

"AttrName" : "热水循环泵运行状态",

"AttrType" : "状态",

"DisplayName" : "热水循环泵运行状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100202000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100202003,

"AttrName" : "热水循环泵手自动模式",

"AttrType" : "状态",

"DisplayName" : "热水循环泵手自动模式",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100202000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100202004,

"AttrName" : "热水循环泵故障报警",

"AttrType" : "告警",

"DisplayName" : "热水循环泵故障报警",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100202000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100202005,

"AttrName" : "热水循环泵水泵进口压力",

"AttrType" : "监测",

"DisplayName" : "热水循环泵水泵进口压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100202000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100202006,

"AttrName" : "热水循环泵水泵出口压力",

"AttrType" : "监测",

"DisplayName" : "热水循环泵水泵出口压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100202000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100202007,

"AttrName" : "热水循环泵频率控制",

"AttrType" : "操作",

"DisplayName" : "热水循环泵频率控制",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100202000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100202008,

"AttrName" : "热水循环泵频率反馈",

"AttrType" : "状态",

"DisplayName" : "热水循环泵频率反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100202000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100203001,

"AttrName" : "锅炉热源系统分集水器压差",

"AttrType" : "监测",

"DisplayName" : "锅炉热源系统分集水器压差",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100203000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100203002,

"AttrName" : "锅炉热源系统总供水压差设定值",

"AttrType" : "操作",

"DisplayName" : "锅炉热源系统总供水压差设定值",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100203000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100203003,

"AttrName" : "锅炉热源系统最不利末端压差设定值",

"AttrType" : "操作",

"DisplayName" : "锅炉热源系统最不利末端压差设定值",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100203000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100203004,

"AttrName" : "锅炉热源系统热水流量",

"AttrType" : "监测",

"DisplayName" : "锅炉热源系统热水流量",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100203000,

"ValueMax" : 10000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "m3/h"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100203005,

"AttrName" : "锅炉热源系统热水总供水温度",

"AttrType" : "监测",

"DisplayName" : "锅炉热源系统热水总供水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100203000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100203006,

"AttrName" : "锅炉热源系统热水总回水温度",

"AttrType" : "监测",

"DisplayName" : "锅炉热源系统热水总回水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100203000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100203007,

"AttrName" : "锅炉热源系统热源机房温度",

"AttrType" : "监测",

"DisplayName" : "锅炉热源系统热源机房温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100203000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100204001,

"AttrName" : "板式换热器阀门开关控制",

"AttrType" : "操作",

"DisplayName" : "板式换热器阀门开关控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100204000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100205001,

"AttrName" : "热水循环泵启停控制",

"AttrType" : "操作",

"DisplayName" : "热水循环泵启停控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100205000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100205002,

"AttrName" : "热水循环泵运行状态",

"AttrType" : "状态",

"DisplayName" : "热水循环泵运行状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100205000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100205003,

"AttrName" : "热水循环泵手自动模式",

"AttrType" : "状态",

"DisplayName" : "热水循环泵手自动模式",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100205000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100205004,

"AttrName" : "热水循环泵故障报警",

"AttrType" : "告警",

"DisplayName" : "热水循环泵故障报警",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100205000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100205005,

"AttrName" : "热水循环泵进口压力",

"AttrType" : "监测",

"DisplayName" : "热水循环泵进口压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100205000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100205006,

"AttrName" : "热水循环泵出口压力",

"AttrType" : "监测",

"DisplayName" : "热水循环泵出口压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100205000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100205007,

"AttrName" : "热水循环泵频率控制",

"AttrType" : "操作",

"DisplayName" : "热水循环泵频率控制",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100205000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100205008,

"AttrName" : "热水循环泵频率反馈",

"AttrType" : "状态",

"DisplayName" : "热水循环泵频率反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100205000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100206001,

"AttrName" : "板式换热站热源系统总供水压差设定值",

"AttrType" : "操作",

"DisplayName" : "板式换热站热源系统总供水压差设定值",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100206000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100206002,

"AttrName" : "板式换热站热源系统最不利末端压差设定值",

"AttrType" : "操作",

"DisplayName" : "板式换热站热源系统最不利末端压差设定值",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100206000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100206003,

"AttrName" : "板式换热站热源系统热水流量",

"AttrType" : "监测",

"DisplayName" : "板式换热站热源系统热水流量",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100206000,

"ValueMax" : 10000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "m3/h"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100206004,

"AttrName" : "板式换热站热源系统热水总供水温度",

"AttrType" : "监测",

"DisplayName" : "板式换热站热源系统热水总供水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100206000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100206005,

"AttrName" : "板式换热站热源系统热水总回水温度",

"AttrType" : "监测",

"DisplayName" : "板式换热站热源系统热水总回水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100206000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100206006,

"AttrName" : "板式换热站热源系统热源机房温度",

"AttrType" : "监测",

"DisplayName" : "板式换热站热源系统热源机房温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100206000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100207001,

"AttrName" : "供回水管网换热站出水温度",

"AttrType" : "监测",

"DisplayName" : "供回水管网换热站出水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100207000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100207002,

"AttrName" : "供回水管网换热站回水温度",

"AttrType" : "监测",

"DisplayName" : "供回水管网换热站回水温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100207000,

"ValueMax" : 100.00,

"ValueMin" : -20.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301001,

"AttrName" : "组合式空调系统启停",

"AttrType" : "操作监测",

"DisplayName" : "系统启停",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301002,

"AttrName" : "组合式空调温度设定",

"AttrType" : "操作监测",

"DisplayName" : "温度设定",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 50.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301003,

"AttrName" : "组合式空调湿度设定",

"AttrType" : "操作监测",

"DisplayName" : "湿度设定",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301004,

"AttrName" : "组合式空调新风温度",

"AttrType" : "监测",

"DisplayName" : "新风温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 50.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301005,

"AttrName" : "组合式空调新风湿度",

"AttrType" : "监测",

"DisplayName" : "新风湿度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301006,

"AttrName" : "组合式空调回风阀",

"AttrType" : "操作监测",

"DisplayName" : "回风阀开度",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301007,

"AttrName" : "组合式空调防冻报警",

"AttrType" : "告警",

"DisplayName" : "防冻报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301008,

"AttrName" : "组合式空调风机压差",

"AttrType" : "监测",

"DisplayName" : "风机压差",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 500.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kbar"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301009,

"AttrName" : "组合式空调高温报警",

"AttrType" : "告警",

"DisplayName" : "高温报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301010,

"AttrName" : "组合式空调送风温度",

"AttrType" : "监测",

"DisplayName" : "送风温度",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 50.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301011,

"AttrName" : "组合式空调送风湿度",

"AttrType" : "监测",

"DisplayName" : "送风湿度",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301012,

"AttrName" : "组合式空调风管压力",

"AttrType" : "监测",

"DisplayName" : "风管压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 500.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kbar"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301013,

"AttrName" : "组合式空调新风阀门",

"AttrType" : "操作监测",

"DisplayName" : "新风阀门",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301014,

"AttrName" : "组合式空调滤网报警",

"AttrType" : "告警",

"DisplayName" : "滤网报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301015,

"AttrName" : "组合式空调冷热水阀给定",

"AttrType" : "操作监测",

"DisplayName" : "冷热水阀给定",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301016,

"AttrName" : "组合式空调冷热水阀反馈",

"AttrType" : "监测",

"DisplayName" : "冷热水阀反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301017,

"AttrName" : "组合式空调加湿阀给定",

"AttrType" : "操作监测",

"DisplayName" : "加湿阀给定",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301018,

"AttrName" : "组合式空调加湿阀反馈",

"AttrType" : "监测",

"DisplayName" : "加湿阀反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301019,

"AttrName" : "组合式空调送风机启停",

"AttrType" : "操作监测",

"DisplayName" : "送风机启停",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301020,

"AttrName" : "组合式空调送风机运行状态",

"AttrType" : "状态",

"DisplayName" : "送风机运行状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : 0,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301021,

"AttrName" : "组合式空调送风机故障",

"AttrType" : "告警",

"DisplayName" : "送风机故障",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : 0,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301022,

"AttrName" : "组合式空调送风机手自动状态",

"AttrType" : "状态",

"DisplayName" : "送风机手自动状态",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : 0,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301023,

"AttrName" : "组合式空调变频器调节",

"AttrType" : "操作监测",

"DisplayName" : "变频器调节",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100301024,

"AttrName" : "组合式空调变频器反馈",

"AttrType" : "监测",

"DisplayName" : "变频器反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301025,

"AttrName" : "组合式空调手自动状态",

"AttrType" : "配置",

"DisplayName" : "手自动状态",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : 0,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100301026,

"AttrName" : "组合式空调自动运行模式",

"AttrType" : "配置",

"DisplayName" : "自动运行模式",

"EnumVals" : "1:夏季工作日；2：夏季休息日；3：冬季工作日；4：冬季休息日",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100301000,

"ValueMax" : 4.00,

"ValueMin" : 1.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100302001,

"AttrName" : "吊顶式空调启停控制",

"AttrType" : "操作监测",

"DisplayName" : "启停控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100302000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100302002,

"AttrName" : "吊顶式空调运行状态",

"AttrType" : "状态",

"DisplayName" : "运行状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100302000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100302003,

"AttrName" : "吊顶式空调手自动模式",

"AttrType" : "状态",

"DisplayName" : "手自动模式",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100302000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100302004,

"AttrName" : "吊顶式空调故障报警",

"AttrType" : "告警",

"DisplayName" : "故障报警",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100302000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 80.00,

"AlarmLow" : 20.00,

"AlarmType" : 0,

"AttrCode" : 100302005,

"AttrName" : "吊顶式空调送风温度",

"AttrType" : "操作监测",

"DisplayName" : "送风温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100302000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100302006,

"AttrName" : "吊顶式空调电动水阀控制",

"AttrType" : "操作监测",

"DisplayName" : "电动水阀控制",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100302000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100302007,

"AttrName" : "吊顶式空调电动水阀反馈",

"AttrType" : "监测",

"DisplayName" : "电动水阀反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100302000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100303001,

"AttrName" : "风机盘管启停控制",

"AttrType" : "操作监测",

"DisplayName" : "风机盘管启停控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100303000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100303002,

"AttrName" : "风机盘管运行状态",

"AttrType" : "状态",

"DisplayName" : "风机盘管运行状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100303000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100303003,

"AttrName" : "风机盘管手自动模式",

"AttrType" : "状态",

"DisplayName" : "风机盘管手自动模式",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100303000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100401001,

"AttrName" : "新风系统启停",

"AttrType" : "操作监测",

"DisplayName" : "系统启停",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100401002,

"AttrName" : "新风温度设定",

"AttrType" : "操作监测",

"DisplayName" : "温度设定",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : 50.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100401003,

"AttrName" : "新风送风温度",

"AttrType" : "操作监测",

"DisplayName" : "送风温度",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : 50.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100401004,

"AttrName" : "新风滤网报警",

"AttrType" : "告警",

"DisplayName" : "滤网报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 0.00,

"AlarmLow" : 0.00,

"AlarmType" : 1,

"AttrCode" : 100401005,

"AttrName" : "新风冷热水阀给定",

"AttrType" : "操作监测",

"DisplayName" : "冷热水阀给定",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 100401006,

"AttrName" : "新风冷热水阀反馈",

"AttrType" : "监测",

"DisplayName" : "冷热水阀反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100401007,

"AttrName" : "新风送风机启停",

"AttrType" : "操作监测",

"DisplayName" : "送风机启停",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100401008,

"AttrName" : "新风送风机运行状态",

"AttrType" : "状态",

"DisplayName" : "送风机运行状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100401009,

"AttrName" : "新风送风机故障",

"AttrType" : "告警",

"DisplayName" : "送风机故障",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100401011,

"AttrName" : "新风送风机手自动状态",

"AttrType" : "配置",

"DisplayName" : "手自动状态",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 100401012,

"AttrName" : "新风机组自动运行模式",

"AttrType" : "配置",

"DisplayName" : "自动运行模式",

"EnumVals" : "1:夏季工作日;2：夏季休息日;3：冬季工作日;4：冬季休息日",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100401000,

"ValueMax" : 4.00,

"ValueMin" : 1.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : 40.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100501001,

"AttrName" : "温度",

"AttrType" : "监测",

"DisplayName" : "温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100501000,

"ValueMax" : 50.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : 100.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100501002,

"AttrName" : "湿度",

"AttrType" : "监测",

"DisplayName" : "湿度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100501000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : 1500.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100501003,

"AttrName" : "CO2浓度",

"AttrType" : "监测",

"DisplayName" : "CO2浓度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100501000,

"ValueMax" : 1500.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "ppm"

}, {

"AlarmHigh" : 200.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100501004,

"AttrName" : "PM2.5",

"AttrType" : "监测",

"DisplayName" : "PM2.5",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 100501000,

"ValueMax" : 300.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "μg/m3"

}, {

"AlarmHigh" : 150.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100501005,

"AttrName" : "噪声",

"AttrType" : "监测",

"DisplayName" : "噪声",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 100501000,

"ValueMax" : 150.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "db"

}, {

"AlarmHigh" : 6000.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100501006,

"AttrName" : "PM10",

"AttrType" : "监测",

"DisplayName" : "PM10",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 100501000,

"ValueMax" : 6000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "ug/m3"

}, {

"AlarmHigh" : 200000.00,

"AlarmLow" : 0.00,

"AlarmType" : 3,

"AttrCode" : 100501007,

"AttrName" : "光照强度",

"AttrType" : "监测",

"DisplayName" : "光照强度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 100501000,

"ValueMax" : 200000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "Lux"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110101001,

"AttrName" : "开关控制",

"AttrType" : "操作",

"DisplayName" : "开关控制",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "IO",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110101002,

"AttrName" : "开关状态",

"AttrType" : "状态",

"DisplayName" : "开关状态",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110101003,

"AttrName" : "开关故障状态",

"AttrType" : "告警",

"DisplayName" : "开关故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110101004,

"AttrName" : "开关控制状态",

"AttrType" : "操作监测",

"DisplayName" : "开关状态",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110102001,

"AttrName" : "开关控制",

"AttrType" : "操作",

"DisplayName" : "开关控制",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "IO",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110102002,

"AttrName" : "开关状态",

"AttrType" : "状态",

"DisplayName" : "开关状态",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110102003,

"AttrName" : "开关故障状态",

"AttrType" : "告警",

"DisplayName" : "开关故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110102004,

"AttrName" : "回路工作状态",

"AttrType" : "状态",

"DisplayName" : "回路工作状态",

"EnumVals" : "0:关闭;1:打开",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110102005,

"AttrName" : "开关控制状态",

"AttrType" : "操作监测",

"DisplayName" : "开关状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110103001,

"AttrName" : "开关控制",

"AttrType" : "操作",

"DisplayName" : "开关控制",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "IO",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 110103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110103002,

"AttrName" : "开关状态",

"AttrType" : "状态",

"DisplayName" : "开关状态",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 110103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110103003,

"AttrName" : "开关故障状态",

"AttrType" : "告警",

"DisplayName" : "开关故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 110103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110103004,

"AttrName" : "回路工作状态",

"AttrType" : "状态",

"DisplayName" : "回路工作状态",

"EnumVals" : "0:关闭;1:打开",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 110103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110103005,

"AttrName" : "开关控制状态",

"AttrType" : "操作监测",

"DisplayName" : "开关状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 110103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110103006,

"AttrName" : "亮度控制状态",

"AttrType" : "操作监测",

"DisplayName" : "亮度控制状态",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 110103000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110103007,

"AttrName" : "亮度控制",

"AttrType" : "操作",

"DisplayName" : "亮度控制",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 110103000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110103008,

"AttrName" : "亮度状态",

"AttrType" : "状态",

"DisplayName" : "亮度状态",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 110103000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 110103009,

"AttrName" : "亮度自动调节",

"AttrType" : "操作",

"DisplayName" : "亮度自动调节",

"EnumVals" : "0:否;1:是",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 110103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120101001,

"AttrName" : "高压进出线电流",

"AttrType" : "监测",

"DisplayName" : "电流",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120101000,

"ValueMax" : 3000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "A"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120101002,

"AttrName" : "高压进出线电压",

"AttrType" : "监测",

"DisplayName" : "电压",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120101000,

"ValueMax" : 750.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kV"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120101003,

"AttrName" : "高压进出线有功功率",

"AttrType" : "监测",

"DisplayName" : "有功功率",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kW"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120101004,

"AttrName" : "高压进出线无功功率",

"AttrType" : "监测",

"DisplayName" : "无功功率",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120101000,

"ValueMax" : 65535.00,

"ValueMin" : -65535.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kvar"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120101005,

"AttrName" : "高压进出线视在功率",

"AttrType" : "监测",

"DisplayName" : "视在功率",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kVA"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120102001,

"AttrName" : "直流屏充放电状态",

"AttrType" : "监测",

"DisplayName" : "充放电状态",

"EnumVals" : "0:充电;1:放电",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120102002,

"AttrName" : "直流屏输出电压",

"AttrType" : "监测",

"DisplayName" : "输出电压",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120102000,

"ValueMax" : 750.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kV"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120102003,

"AttrName" : "直流屏累计放电次数",

"AttrType" : "监测",

"DisplayName" : "累计放电次数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120102000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120102004,

"AttrName" : "直流屏充电电压",

"AttrType" : "监测",

"DisplayName" : "充电电压",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120102000,

"ValueMax" : 750.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kV"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120102005,

"AttrName" : "直流屏电池温度",

"AttrType" : "监测",

"DisplayName" : "电池温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120102000,

"ValueMax" : 70.00,

"ValueMin" : 20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120103001,

"AttrName" : "变压器铁芯线圈温度",

"AttrType" : "监测",

"DisplayName" : "铁芯线圈温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120103000,

"ValueMax" : 70.00,

"ValueMin" : 20.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120103002,

"AttrName" : "变压器散热风机状态",

"AttrType" : "状态",

"DisplayName" : "散热风机状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120103003,

"AttrName" : "变压器高温报警方式",

"AttrType" : "监测",

"DisplayName" : "高温报警方式",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120104001,

"AttrName" : "低压电进线电流",

"AttrType" : "监测",

"DisplayName" : "电流",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120104000,

"ValueMax" : 3000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "A"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120104002,

"AttrName" : "低压电进线电压",

"AttrType" : "监测",

"DisplayName" : "电压",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120104000,

"ValueMax" : 10000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "V"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120104003,

"AttrName" : "低压电进线有功功率",

"AttrType" : "监测",

"DisplayName" : "有功功率",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120104000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kW"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120104004,

"AttrName" : "低压电进线功率因数",

"AttrType" : "监测",

"DisplayName" : "功率因数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120104000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : 2,

"ValueType" : "float",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120104005,

"AttrName" : "低压电进线谐波率",

"AttrType" : "监测",

"DisplayName" : "谐波率",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120104000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 2,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120104006,

"AttrName" : "低压电进线用电量",

"AttrType" : "监测",

"DisplayName" : "用电量",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120104000,

"ValueMax" : 21474836.47,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kWh"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120105001,

"AttrName" : "低压电出线电流",

"AttrType" : "监测",

"DisplayName" : "电流",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120105000,

"ValueMax" : 3000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "A"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120105002,

"AttrName" : "低压电出线电压",

"AttrType" : "监测",

"DisplayName" : "电压",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120105000,

"ValueMax" : 10000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "V"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120105003,

"AttrName" : "低压电出线有功功率",

"AttrType" : "监测",

"DisplayName" : "有功功率",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120105000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kW"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120105004,

"AttrName" : "低压电出线功率因数",

"AttrType" : "监测",

"DisplayName" : "功率因数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120105000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : 2,

"ValueType" : "float",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120105005,

"AttrName" : "低压电出线用电量",

"AttrType" : "监测",

"DisplayName" : "用电量",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120105000,

"ValueMax" : 21474836.47,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kWh"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120106001,

"AttrName" : "柴油发电机输出电流",

"AttrType" : "监测",

"DisplayName" : "输出电流",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120106000,

"ValueMax" : 3000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "A"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120106002,

"AttrName" : "柴油发电机输出电压",

"AttrType" : "监测",

"DisplayName" : "输出电压",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120106000,

"ValueMax" : 10000.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "V"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120106003,

"AttrName" : "柴油发电机频率",

"AttrType" : "监测",

"DisplayName" : "频率",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120106000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120106004,

"AttrName" : "柴油发电机电量",

"AttrType" : "监测",

"DisplayName" : "电量",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120106000,

"ValueMax" : 21474836.47,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "kWh"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120106005,

"AttrName" : "柴油发电机水温",

"AttrType" : "监测",

"DisplayName" : "水温",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120106000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120106006,

"AttrName" : "柴油发电机电池",

"AttrType" : "监测",

"DisplayName" : "电池状态",

"EnumVals" : "0:正常;1:亏电",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120106000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120106007,

"AttrName" : "柴油发电机状态",

"AttrType" : "状态",

"DisplayName" : "状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120106000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120106008,

"AttrName" : "柴油发电机故障状态",

"AttrType" : "告警",

"DisplayName" : "故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120106000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120107001,

"AttrName" : "UPS/EPS充放电状态",

"AttrType" : "状态",

"DisplayName" : "充放电状态",

"EnumVals" : "0:充电;1:放电",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120107002,

"AttrName" : "UPS/EPS电池失效状态",

"AttrType" : "状态",

"DisplayName" : "电池失效状态",

"EnumVals" : "0:正常;1:失效",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120107003,

"AttrName" : "UPS/EPS输出电压",

"AttrType" : "监测",

"DisplayName" : "输出电压",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120107000,

"ValueMax" : 750.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kV"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120107004,

"AttrName" : "UPS/EPS状态异常报警",

"AttrType" : "告警",

"DisplayName" : "状态异常",

"EnumVals" : "0:启动失败;1:无法同步;2:短路;3:电池失效;4:电压异常",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120107000,

"ValueMax" : 128.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120108001,

"AttrName" : "配电室温度",

"AttrType" : "监测",

"DisplayName" : "温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120108000,

"ValueMax" : 70.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120108002,

"AttrName" : "配电室湿度",

"AttrType" : "监测",

"DisplayName" : "湿度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120108000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120109001,

"AttrName" : "功率补偿无功电流",

"AttrType" : "监测",

"DisplayName" : "无功电流",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120109000,

"ValueMax" : 3000.00,

"ValueMin" : -3000.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "A"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120109002,

"AttrName" : "功率补偿无功功率",

"AttrType" : "监测",

"DisplayName" : "无功功率",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120109000,

"ValueMax" : 65535.00,

"ValueMin" : -65535.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "kvar"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 120109003,

"AttrName" : "功率补偿功率因数",

"AttrType" : "监测",

"DisplayName" : "功率因数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120109000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : 2,

"ValueType" : "float",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120109004,

"AttrName" : "功率补偿补偿器温度",

"AttrType" : "监测",

"DisplayName" : "补偿器温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120109000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 120109005,

"AttrName" : "功率补偿状态",

"AttrType" : "监测",

"DisplayName" : "补偿状态",

"EnumVals" : "0:断开;1:投入",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 120109000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130101001,

"AttrName" : "生活水泵启停状态",

"AttrType" : "状态",

"DisplayName" : "启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130101002,

"AttrName" : "生活水泵手自动状态",

"AttrType" : "状态",

"DisplayName" : "手自动状态",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130101003,

"AttrName" : "生活水泵故障状态",

"AttrType" : "告警",

"DisplayName" : "故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130101004,

"AttrName" : "生活水泵速度变频反馈",

"AttrType" : "监测",

"DisplayName" : "速度变频反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "int",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 130101005,

"AttrName" : "生活水泵管网压力",

"AttrType" : "监测",

"DisplayName" : "管网压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130101000,

"ValueMax" : 1000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 130101006,

"AttrName" : "生活水泵减压阀前后压力",

"AttrType" : "监测",

"DisplayName" : "减压阀前后压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130101000,

"ValueMax" : 1000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130101007,

"AttrName" : "生活水泵定压报警",

"AttrType" : "告警",

"DisplayName" : "定压报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130102001,

"AttrName" : "不锈钢水箱高水位报警",

"AttrType" : "告警",

"DisplayName" : "高水位报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130102002,

"AttrName" : "不锈钢水箱低水位报警",

"AttrType" : "告警",

"DisplayName" : "低水位报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 130103001,

"AttrName" : "机房温度",

"AttrType" : "监测",

"DisplayName" : "机房温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130103000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130104001,

"AttrName" : "污水坑泵启停状态",

"AttrType" : "状态",

"DisplayName" : "启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130104002,

"AttrName" : "污水坑泵故障状态",

"AttrType" : "告警",

"DisplayName" : "故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130104003,

"AttrName" : "污水坑泵手自动状态",

"AttrType" : "状态",

"DisplayName" : "手自动状态",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130105001,

"AttrName" : "污水集水池高水位报警点",

"AttrType" : "告警",

"DisplayName" : "高水位报警点",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130105000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130106001,

"AttrName" : "隔油池超高水位报警点",

"AttrType" : "告警",

"DisplayName" : "超高水位报警点",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130106000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130107001,

"AttrName" : "冷却水补水水泵启停状态",

"AttrType" : "状态",

"DisplayName" : "启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130107002,

"AttrName" : "冷却水补水水泵手自动状态",

"AttrType" : "状态",

"DisplayName" : "手自动状态",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130107003,

"AttrName" : "冷却水补水水泵故障状态",

"AttrType" : "告警",

"DisplayName" : "故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130107004,

"AttrName" : "冷却水补水水泵速度变频反馈",

"AttrType" : "监测",

"DisplayName" : "速度变频反馈",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130107000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "int",

"ValueUnit" : "Hz"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130107005,

"AttrName" : "冷却水补水水泵管网压力",

"AttrType" : "监测",

"DisplayName" : "管网压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130107000,

"ValueMax" : 1000.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130108001,

"AttrName" : "雨水提升泵启停状态",

"AttrType" : "状态",

"DisplayName" : "启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130108000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130108002,

"AttrName" : "雨水提升泵手自动状态",

"AttrType" : "状态",

"DisplayName" : "手自动状态",

"EnumVals" : "0:手动;1:自动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130108000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130108003,

"AttrName" : "雨水提升泵故障状态",

"AttrType" : "告警",

"DisplayName" : "故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130108000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 130109001,

"AttrName" : "雨水回收池流量监测",

"AttrType" : "监测",

"DisplayName" : "流量监测",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130109000,

"ValueMax" : 50.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "m3/h"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 130109002,

"AttrName" : "雨水回收池低液位报警",

"AttrType" : "告警",

"DisplayName" : "低液位报警",

"EnumVals" : "0:正常;1:报警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130109000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 130110001,

"AttrName" : "消火栓水泵出口环管处压力",

"AttrType" : "监测",

"DisplayName" : "出口环管处压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130110000,

"ValueMax" : 1000.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 130111001,

"AttrName" : "喷淋水泵出口环管处压力",

"AttrType" : "监测",

"DisplayName" : "出口环管处压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130111000,

"ValueMax" : 1000.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 130112001,

"AttrName" : "消防水炮泵出口环管处压力",

"AttrType" : "监测",

"DisplayName" : "出口环管处压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130112000,

"ValueMax" : 1000.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 130113001,

"AttrName" : "防护冷却水泵出口环管处压力",

"AttrType" : "监测",

"DisplayName" : "出口环管处压力",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 130113000,

"ValueMax" : 1000.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "mH2O"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 140101001,

"AttrName" : "直梯启停状态",

"AttrType" : "状态",

"DisplayName" : "直梯启停状态",

"EnumVals" : "0:停用;1:启用",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140101000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 140101002,

"AttrName" : "直梯楼层信息",

"AttrType" : "监测",

"DisplayName" : "直梯楼层信息",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140101000,

"ValueMax" : 200.00,

"ValueMin" : -100.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "层"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 140101003,

"AttrName" : "直梯运行状态",

"AttrType" : "告警",

"DisplayName" : "直梯运行状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 140101004,

"AttrName" : "直梯上下行状态",

"AttrType" : "状态",

"DisplayName" : "直梯上下行状态",

"EnumVals" : "0:上行;1:下行",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 140102001,

"AttrName" : "扶梯启停状态",

"AttrType" : "状态",

"DisplayName" : "扶梯启停状态",

"EnumVals" : "0:停用;1:启用",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 140102002,

"AttrName" : "扶梯运行状态",

"AttrType" : "告警",

"DisplayName" : "扶梯运行状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 140102003,

"AttrName" : "扶梯上下行状态",

"AttrType" : "状态",

"DisplayName" : "扶梯上下行状态",

"EnumVals" : "0:上行;1:下行",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 35.00,

"AlarmLow" : 5.00,

"AlarmType" : 3,

"AttrCode" : 140103001,

"AttrName" : "电梯机房温度",

"AttrType" : "监测",

"DisplayName" : "电梯机房温度",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140103000,

"ValueMax" : 60.00,

"ValueMin" : -30.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 140104001,

"AttrName" : "电梯底坑抽水泵状态",

"AttrType" : "状态",

"DisplayName" : "电梯底坑抽水泵状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 140104002,

"AttrName" : "电梯底坑液位报警",

"AttrType" : "告警",

"DisplayName" : "电梯底坑液位报警",

"EnumVals" : "0:正常;1:高液位",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 140104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 150101001,

"AttrName" : "电表读数",

"AttrType" : "监测",

"DisplayName" : "电表读数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 150101000,

"ValueMax" : 21474836.47,

"ValueMin" : 0.00,

"ValuePrecision" : 2,

"ValueType" : "float",

"ValueUnit" : "kWh"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 150101002,

"AttrName" : "电表故障状态",

"AttrType" : "告警",

"DisplayName" : "电表故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 150101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 150201001,

"AttrName" : "水表读数",

"AttrType" : "监测",

"DisplayName" : "水表读数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 150201000,

"ValueMax" : 21474836.47,

"ValueMin" : 0.00,

"ValuePrecision" : 2,

"ValueType" : "float",

"ValueUnit" : "m3"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 150201002,

"AttrName" : "水表故障状态",

"AttrType" : "告警",

"DisplayName" : "水表故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 150201000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 150301001,

"AttrName" : "气表读数",

"AttrType" : "监测",

"DisplayName" : "气表读数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 150301000,

"ValueMax" : 21474836.47,

"ValueMin" : 0.00,

"ValuePrecision" : 2,

"ValueType" : "float",

"ValueUnit" : "m3"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 150301002,

"AttrName" : "气表故障状态",

"AttrType" : "告警",

"DisplayName" : "气表故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 150301000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 160101001,

"AttrName" : "布撤防状态",

"AttrType" : "操作监测",

"DisplayName" : "布撤防状态",

"EnumVals" : "0:布防;1:撤防",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 160101000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 160101002,

"AttrName" : "入侵告警状态",

"AttrType" : "告警",

"DisplayName" : "入侵告警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 160101000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 170101001,

"AttrName" : "巡更点是否在线",

"AttrType" : "状态",

"DisplayName" : "是否在线",

"EnumVals" : "0:在线;1:离线",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 170101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 170101002,

"AttrName" : "巡更点工作状态",

"AttrType" : "状态",

"DisplayName" : "工作状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 170101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 180101001,

"AttrName" : "门禁控制器启停状态",

"AttrType" : "状态",

"DisplayName" : "门禁控制器启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 180101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 180101002,

"AttrName" : "门禁控制器告警状态",

"AttrType" : "告警",

"DisplayName" : "门禁控制器告警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 180101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 180102001,

"AttrName" : "门禁读卡器启停状态",

"AttrType" : "状态",

"DisplayName" : "门禁读卡器启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 180102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 180102002,

"AttrName" : "门禁读卡器告警状态",

"AttrType" : "告警",

"DisplayName" : "门禁读卡器告警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 180102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 180103001,

"AttrName" : "门禁门锁开关控制",

"AttrType" : "操作",

"DisplayName" : "门禁门锁开关控制",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "IO",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 180103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 180103002,

"AttrName" : "门禁门锁状态",

"AttrType" : "状态",

"DisplayName" : "门禁门锁状态",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 180103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 180103003,

"AttrName" : "门禁门锁告警状态",

"AttrType" : "告警",

"DisplayName" : "门禁门锁告警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 180103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101001,

"AttrName" : "摄像机工作状态",

"AttrType" : "状态",

"DisplayName" : "摄像机工作状态",

"EnumVals" : "0:离线;1:在线",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101002,

"AttrName" : "摄像机告警状态",

"AttrType" : "配置",

"DisplayName" : "摄像机告警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101003,

"AttrName" : "摄像机型号",

"AttrType" : "配置",

"DisplayName" : "摄像机型号",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101004,

"AttrName" : "摄像机端口号",

"AttrType" : "配置",

"DisplayName" : "摄像机端口号",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101005,

"AttrName" : "摄像机用户名",

"AttrType" : "配置",

"DisplayName" : "摄像机用户名",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101006,

"AttrName" : "摄像机密码",

"AttrType" : "配置",

"DisplayName" : "摄像机密码",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101007,

"AttrName" : "摄像机序列号",

"AttrType" : "配置",

"DisplayName" : "摄像机序列号",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101008,

"AttrName" : "摄像机联系人",

"AttrType" : "配置",

"DisplayName" : "摄像机联系人",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101009,

"AttrName" : "摄像机联系人号码",

"AttrType" : "配置",

"DisplayName" : "摄像机联系人号码",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101010,

"AttrName" : "摄像机权限",

"AttrType" : "配置",

"DisplayName" : "摄像机权限",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101011,

"AttrName" : "实时监控",

"AttrType" : "操作",

"DisplayName" : "实时监控",

"EnumVals" : " ",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 0,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101012,

"AttrName" : "视频轮巡",

"AttrType" : "操作",

"DisplayName" : "视频轮巡",

"EnumVals" : " ",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 0,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101013,

"AttrName" : "点间巡航",

"AttrType" : "操作",

"DisplayName" : "点间巡航",

"EnumVals" : " ",

"InfoPoint" : "O ",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 0,

"OwnerCode" : 190101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190101014,

"AttrName" : "摄像机类型",

"AttrType" : "配置",

"DisplayName" : "摄像机类型",

"EnumVals" : "0:枪机;1:球机;2:半球机;3:枪球一体机",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 0,

"OwnerCode" : 190101000,

"ValueMax" : 3.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190102001,

"AttrName" : "矩阵设备用户名",

"AttrType" : "配置",

"DisplayName" : "矩阵设备用户名",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190102002,

"AttrName" : "矩阵设备密码",

"AttrType" : "配置",

"DisplayName" : "矩阵设备密码",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190102003,

"AttrName" : "矩阵通道数目",

"AttrType" : "配置",

"DisplayName" : "矩阵通道数目",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190102000,

"ValueMax" : 128.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190102004,

"AttrName" : "矩阵设备工作状态",

"AttrType" : "状态",

"DisplayName" : "矩阵设备工作状态",

"EnumVals" : "0:离线;1:在线",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190102005,

"AttrName" : "矩阵设备告警状态",

"AttrType" : "配置",

"DisplayName" : "矩阵设备告警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190103001,

"AttrName" : "大屏设备工作状态",

"AttrType" : "状态",

"DisplayName" : "大屏设备工作状态",

"EnumVals" : "0:离线;1:在线",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190103002,

"AttrName" : "大屏设备告警状态",

"AttrType" : "配置",

"DisplayName" : "大屏设备告警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190104001,

"AttrName" : "硬盘录像机工作状态",

"AttrType" : "状态",

"DisplayName" : "硬盘录像机工作状态",

"EnumVals" : "0:离线;1:在线",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190104002,

"AttrName" : "硬盘录像机告警状态",

"AttrType" : "配置",

"DisplayName" : "硬盘录像机告警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190104003,

"AttrName" : "硬盘录像机序列号",

"AttrType" : "配置",

"DisplayName" : "硬盘录像机序列号",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 190104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190104004,

"AttrName" : "硬盘录像机通道号",

"AttrType" : "配置",

"DisplayName" : "硬盘录像机通道号",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190104000,

"ValueMax" : 255.00,

"ValueMin" : 1.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190105001,

"AttrName" : "磁盘阵列工作状态",

"AttrType" : "状态",

"DisplayName" : "磁盘阵列工作状态",

"EnumVals" : "0:离线;1:在线",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190105000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 190105002,

"AttrName" : "磁盘阵列告警状态",

"AttrType" : "配置",

"DisplayName" : "磁盘阵列告警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 190105000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 200100001,

"AttrName" : "广播音源数量",

"AttrType" : "状态",

"DisplayName" : "广播音源设备",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 200100000,

"ValueMax" : 5.00,

"ValueMin" : 1.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 200100002,

"AttrName" : "当前播放音源",

"AttrType" : "状态",

"DisplayName" : "当前正在播放的音源设备",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 200100000,

"ValueMax" : 5.00,

"ValueMin" : 1.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : 0,

"AttrCode" : 200101001,

"AttrName" : "设备音量",

"AttrType" : "操作",

"DisplayName" : "设备音量",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 200101000,

"ValueMax" : 60.00,

"ValueMin" : 1.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 200101002,

"AttrName" : "设备运行状态",

"AttrType" : "状态",

"DisplayName" : "设备运行状态",

"EnumVals" : "0:离线;1:空闲;2:播放",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 200101000,

"ValueMax" : 2.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 200101003,

"AttrName" : "播放节目",

"AttrType" : "状态",

"DisplayName" : "播放节目",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 200101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 200101004,

"AttrName" : "播放文件",

"AttrType" : "状态",

"DisplayName" : "播放文件",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 200101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 200101005,

"AttrName" : "播放任务",

"AttrType" : "操作",

"DisplayName" : "广播设备播放任务",

"EnumVals" : "0:无任务;1:有任务",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 200101000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101001,

"AttrName" : "屏幕启停状态",

"AttrType" : "操作监测",

"DisplayName" : "屏幕启停状态",

"EnumVals" : "0:关闭;1:开启",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101002,

"AttrName" : "屏幕运行状态",

"AttrType" : "告警",

"DisplayName" : "屏幕运行状态",

"EnumVals" : "0:正常;1:离线",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101003,

"AttrName" : "屏幕温度",

"AttrType" : "监测",

"DisplayName" : "屏幕温度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : 70.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "℃"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101004,

"AttrName" : "屏幕亮度",

"AttrType" : "操作监测",

"DisplayName" : "屏幕亮度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "int",

"ValueUnit" : "cd/m2"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101005,

"AttrName" : "屏幕类型",

"AttrType" : "状态",

"DisplayName" : "屏幕类型",

"EnumVals" : "0:全彩屏;1:双色屏",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101006,

"AttrName" : "屏幕宽度",

"AttrType" : "配置",

"DisplayName" : "屏幕宽度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : 1,

"ValueType" : "int",

"ValueUnit" : "cm"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101007,

"AttrName" : "屏幕高度",

"AttrType" : "配置",

"DisplayName" : "屏幕高度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : 1,

"ValueType" : "int",

"ValueUnit" : "cm"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101008,

"AttrName" : "设备音量",

"AttrType" : "监测",

"DisplayName" : "设备音量",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101009,

"AttrName" : "当前播放频道",

"AttrType" : "监测",

"DisplayName" : "当前播放频道",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210101010,

"AttrName" : "当前播放节目",

"AttrType" : "监测",

"DisplayName" : "当前播放节目",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210102001,

"AttrName" : "LED主机启停状态",

"AttrType" : "状态",

"DisplayName" : "LED主机启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210102002,

"AttrName" : "LED主机运行状态",

"AttrType" : "告警",

"DisplayName" : "LED主机运行状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210102003,

"AttrName" : "LED主机播放节目选择",

"AttrType" : "操作",

"DisplayName" : "LED主机播放节目选择",

"EnumVals" : "",

"InfoPoint" : "IO",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210102000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 210102004,

"AttrName" : "LED主机播放状态反馈",

"AttrType" : "状态",

"DisplayName" : "LED主机播放状态反馈",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 210102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 220101001,

"AttrName" : "启停状态",

"AttrType" : "状态",

"DisplayName" : "启停状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 220101002,

"AttrName" : "运行状态",

"AttrType" : "配置",

"DisplayName" : "运行状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 220101003,

"AttrName" : "客流摄像机端口号",

"AttrType" : "配置",

"DisplayName" : "客流摄像机端口号",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 220101004,

"AttrName" : "客流摄像机用户名",

"AttrType" : "配置",

"DisplayName" : "客流摄像机用户名",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 220101005,

"AttrName" : "客流量",

"AttrType" : "监测",

"DisplayName" : "监控设备上报某个时段内的客流",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 220101006,

"AttrName" : "客流摄像机密码",

"AttrType" : "配置",

"DisplayName" : "客流摄像机密码",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 220101008,

"AttrName" : "进入人数",

"AttrType" : "监测",

"DisplayName" : "监测点进入人数",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "人数"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 220101009,

"AttrName" : "退出人数",

"AttrType" : "监测",

"DisplayName" : "监测点退出人数",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "人数"

}, {

"AlarmHigh" : 10000.00,

"AlarmLow" : 5000.00,

"AlarmType" : 1,

"AttrCode" : 220101010,

"AttrName" : "场内人数",

"AttrType" : "监测",

"DisplayName" : "监测点场内人数",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "人数"

}, {

"AlarmHigh" : 20000.00,

"AlarmLow" : 10000.00,

"AlarmType" : 1,

"AttrCode" : 220101011,

"AttrName" : "累计客流",

"AttrType" : "监测",

"DisplayName" : "当天某个时间点的累计客流",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 220101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "人数"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230000001,

"AttrName" : "子系统车位总数",

"AttrType" : "配置",

"DisplayName" : "子系统车位总数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230000000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "个"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230000002,

"AttrName" : "子系统剩余车位数",

"AttrType" : "监测",

"DisplayName" : "子系统剩余车位数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230000000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "个"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230100001,

"AttrName" : "停车管理模块车位总数",

"AttrType" : "配置",

"DisplayName" : "停车管理模块车位总数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230100000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "个"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230100002,

"AttrName" : "停车管理模块剩余车位数",

"AttrType" : "监测",

"DisplayName" : "停车管理模块剩余车位数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230100000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "个"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230101001,

"AttrName" : "道闸运行状态",

"AttrType" : "状态",

"DisplayName" : "道闸运行状态",

"EnumVals" : "0:运行;1:落锁",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230101002,

"AttrName" : "道闸故障状态",

"AttrType" : "告警",

"DisplayName" : "道闸故障状态",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : 0.00,

"AlarmLow" : 0.00,

"AlarmType" : -1,

"AttrCode" : 230102001,

"AttrName" : "车位状态",

"AttrType" : "状态",

"DisplayName" : "车位状态",

"EnumVals" : "0:无车;1:有车",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230102000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230102002,

"AttrName" : "车位类型",

"AttrType" : "配置",

"DisplayName" : "车位类型",

"EnumVals" : "0:普通车位;1:固定车位;2:临时车位;3:VIP车位",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230102000,

"ValueMax" : 3.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "enum",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230102003,

"AttrName" : "车牌号码",

"AttrType" : "监测",

"DisplayName" : "车位停车车牌",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230102004,

"AttrName" : "停车时间",

"AttrType" : "监测",

"DisplayName" : "停车时间",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230102005,

"AttrName" : "抓拍图像",

"AttrType" : "监测",

"DisplayName" : "抓拍图像",

"EnumVals" : " ",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230103001,

"AttrName" : "车道是否车卡一致",

"AttrType" : "监测",

"DisplayName" : "是否车卡一致",

"EnumVals" : "0:不是;1:是",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230103002,

"AttrName" : "车道是否单进单出",

"AttrType" : "监测",

"DisplayName" : "是否单进单出",

"EnumVals" : "0:不是;1:是",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 230103003,

"AttrName" : "车道临时车放行方式",

"AttrType" : "监测",

"DisplayName" : "临时车放行方式",

"EnumVals" : "0:手动放行;1:自动放行",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 230103000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240101001,

"AttrName" : "感温火灾探测器工作状态",

"AttrType" : "状态",

"DisplayName" : "感温火灾探测器工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240101002,

"AttrName" : "感温火灾探测器报警状态",

"AttrType" : "告警",

"DisplayName" : "感温火灾探测器报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240102001,

"AttrName" : "感烟火灾探测器工作状态",

"AttrType" : "状态",

"DisplayName" : "感烟火灾探测器工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240102002,

"AttrName" : "感烟火灾探测器报警状态",

"AttrType" : "告警",

"DisplayName" : "感烟火灾探测器报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240103001,

"AttrName" : "感光火灾探测器工作状态",

"AttrType" : "状态",

"DisplayName" : "感光火灾探测器工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240103002,

"AttrName" : "感光火灾探测器报警状态",

"AttrType" : "告警",

"DisplayName" : "感光火灾探测器报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240103000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240104001,

"AttrName" : "可燃气体探测器工作状态",

"AttrType" : "状态",

"DisplayName" : "可燃气体探测器工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240104002,

"AttrName" : "可燃气体探测器报警状态",

"AttrType" : "告警",

"DisplayName" : "可燃气体探测器报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240104000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240105001,

"AttrName" : "复合火灾探测器工作状态",

"AttrType" : "状态",

"DisplayName" : "复合火灾探测器工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240105000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240105002,

"AttrName" : "复合火灾探测器报警状态",

"AttrType" : "告警",

"DisplayName" : "复合火灾探测器报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240105000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240106001,

"AttrName" : "手动火灾报警按钮工作状态",

"AttrType" : "状态",

"DisplayName" : "手动火灾报警按钮工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240106000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240106002,

"AttrName" : "手动火灾报警按钮报警状态",

"AttrType" : "告警",

"DisplayName" : "手动火灾报警按钮报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240106000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240107001,

"AttrName" : "火灾报警控制器工作状态",

"AttrType" : "状态",

"DisplayName" : "火灾报警控制器工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240107002,

"AttrName" : "火灾报警控制器报警状态",

"AttrType" : "告警",

"DisplayName" : "火灾报警控制器报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240107003,

"AttrName" : "火灾报警控制器备电自动转换",

"AttrType" : "状态",

"DisplayName" : "火灾报警控制器备电自动转换",

"EnumVals" : "0:市电;1:备电",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240107004,

"AttrName" : "火灾报警控制器备用电源充电",

"AttrType" : "状态",

"DisplayName" : "火灾报警控制器备用电源充电",

"EnumVals" : "0:未充电;1:充电",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240107005,

"AttrName" : "火灾报警控制器电源故障监测",

"AttrType" : "告警",

"DisplayName" : "火灾报警控制器电源故障监测",

"EnumVals" : "0:正常;1:故障",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240107006,

"AttrName" : "火灾报警控制器电µ源工作状态",

"AttrType" : "状态",

"DisplayName" : "火灾报警控制器电源工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240107007,

"AttrName" : "火灾报警控制器声光报警",

"AttrType" : "告警",

"DisplayName" : "火灾报警控制器声光报警",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240107008,

"AttrName" : "火灾报警控制器时钟单元",

"AttrType" : "状态",

"DisplayName" : "火灾报警控制器时钟单元",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240107009,

"AttrName" : "火灾报警控制器声报警音响消音",

"AttrType" : "状态",

"DisplayName" : "火灾报警控制器声报警音响消音",

"EnumVals" : "0:正常;1:消音",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240107000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240108001,

"AttrName" : "输入输出模块工作状态",

"AttrType" : "状态",

"DisplayName" : "输入输出模块工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240108000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240108002,

"AttrName" : "输入输出模块报警状态",

"AttrType" : "告警",

"DisplayName" : "输入输出模块报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240108000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240109001,

"AttrName" : "水流指示器工作状态",

"AttrType" : "状态",

"DisplayName" : "水流指示器工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240109000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240109002,

"AttrName" : "水流指示器报警状态",

"AttrType" : "告警",

"DisplayName" : "水流指示器报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240109000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240110001,

"AttrName" : "阀门限位器工作状态",

"AttrType" : "状态",

"DisplayName" : "阀门限位器工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240110000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240110002,

"AttrName" : "阀门限位器报警状态",

"AttrType" : "告警",

"DisplayName" : "阀门限位器报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240110000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240111001,

"AttrName" : "压力检测器工作状态",

"AttrType" : "状态",

"DisplayName" : "压力检测器工作状态",

"EnumVals" : "0:启动;1:停止",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240111000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240111002,

"AttrName" : "压力检测器报警状态",

"AttrType" : "告警",

"DisplayName" : "压力检测器报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240111000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240112001,

"AttrName" : "水力警铃工作状态",

"AttrType" : "状态",

"DisplayName" : "水力警铃工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240112000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240112002,

"AttrName" : "水力警铃报警状态",

"AttrType" : "告警",

"DisplayName" : "水力警铃报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240112000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240113001,

"AttrName" : "压力开关工作状态",

"AttrType" : "状态",

"DisplayName" : "压力开关工作状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240113000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 240113002,

"AttrName" : "压力开关报警状态",

"AttrType" : "告警",

"DisplayName" : "压力开关报警状态",

"EnumVals" : "0:正常;1:告警",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 240113000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 250101003,

"AttrName" : "围墙机开关状态",

"AttrType" : "监测",

"DisplayName" : "围墙机开关状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "1",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 250101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 250101004,

"AttrName" : "围墙机开关控制",

"AttrType" : "操作",

"DisplayName" : "围墙机开关控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "1",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 250101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 250101005,

"AttrName" : "围墙机进出门方向",

"AttrType" : "配置",

"DisplayName" : "围墙机进出门方向",

"EnumVals" : "0:进;1:出",

"InfoPoint" : "1",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 250101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 250102003,

"AttrName" : "门口主机开关状态",

"AttrType" : "监测",

"DisplayName" : "门口主机开关状态",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "1",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 250102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 250102004,

"AttrName" : "门口主机开关控制",

"AttrType" : "操作",

"DisplayName" : "门口主机开关控制",

"EnumVals" : "0:停止;1:启动",

"InfoPoint" : "1",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 250102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 250102005,

"AttrName" : "门口主机出门方向",

"AttrType" : "配置",

"DisplayName" : "门口主机出门方向",

"EnumVals" : "0:进;1:出",

"InfoPoint" : "1",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 250102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : null

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101001,

"AttrName" : "路灯经度",

"AttrType" : "配置",

"DisplayName" : "路灯经度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101002,

"AttrName" : "路灯纬度",

"AttrType" : "配置",

"DisplayName" : "路灯维度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101003,

"AttrName" : "路灯材料",

"AttrType" : "配置",

"DisplayName" : "路灯材料",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101004,

"AttrName" : "路灯型号",

"AttrType" : "配置",

"DisplayName" : "路灯型号",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101005,

"AttrName" : "路灯类型",

"AttrType" : "配置",

"DisplayName" : "路灯类型",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101006,

"AttrName" : "路灯重量",

"AttrType" : "配置",

"DisplayName" : "路灯重量",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "kg"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101007,

"AttrName" : "路灯高度",

"AttrType" : "配置",

"DisplayName" : "路灯高度",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "float",

"ValueUnit" : "m"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101008,

"AttrName" : "路灯所属省",

"AttrType" : "配置",

"DisplayName" : "灯杆所属省",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101009,

"AttrName" : "路灯所属市",

"AttrType" : "配置",

"DisplayName" : "灯杆所属市",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101010,

"AttrName" : "路灯所属城区",

"AttrType" : "配置",

"DisplayName" : "灯杆所属城区",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101011,

"AttrName" : "路灯所属街道",

"AttrType" : "配置",

"DisplayName" : "灯杆所属街道",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101012,

"AttrName" : "安装时间",

"AttrType" : "配置",

"DisplayName" : "安装时间",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "datatime",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 260101013,

"AttrName" : "路灯所属社区",

"AttrType" : "配置",

"DisplayName" : "灯杆所属社区",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 260101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 270101001,

"AttrName" : "充电类型",

"AttrType" : "配置",

"DisplayName" : "设备类型",

"EnumVals" : "0:快充;1:慢充",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 270101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 270101002,

"AttrName" : "启用状态",

"AttrType" : "状态",

"DisplayName" : "启用状态",

"EnumVals" : "0:未启用;1:启用",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 270101000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 270101003,

"AttrName" : "P1充电端口名称",

"AttrType" : "配置",

"DisplayName" : "P1充电端口名称",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 270101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 270101004,

"AttrName" : "P1充电端口状态",

"AttrType" : "状态",

"DisplayName" : "P1充电端口状态",

"EnumVals" : "0:禁用;1:空闲;2:已插枪;3:正在充电;4:充电已结束;5:车位被占用;6:故障或维修中",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 270101000,

"ValueMax" : 6.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 270101005,

"AttrName" : "P2充电端口名称",

"AttrType" : "配置",

"DisplayName" : "P2充电端口名称",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 270101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 270101006,

"AttrName" : "P2充电端口状态",

"AttrType" : "状态",

"DisplayName" : "P2充电端口状态",

"EnumVals" : "0:禁用;1:空闲;2:已插枪;3:正在充电;4:充电已结束;5:车位被占用;6:故障或维修中",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 270101000,

"ValueMax" : 6.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 270101007,

"AttrName" : "P3充电端口名称",

"AttrType" : "配置",

"DisplayName" : "P3充电端口名称",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 270101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 270101008,

"AttrName" : "P3充电端口状态",

"AttrType" : "状态",

"DisplayName" : "P3充电端口状态",

"EnumVals" : "0:禁用;1:空闲;2:已插枪;3:正在充电;4:充电已结束;5:车位被占用;6:故障或维修中",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 270101000,

"ValueMax" : 6.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101001,

"AttrName" : "端口号",

"AttrType" : "配置",

"DisplayName" : "端口号",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : 65535.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101002,

"AttrName" : "用户名",

"AttrType" : "配置",

"DisplayName" : "用户名",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101003,

"AttrName" : "密码",

"AttrType" : "配置",

"DisplayName" : "密码",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101004,

"AttrName" : "监控状态",

"AttrType" : "状态",

"DisplayName" : "监控状态",

"EnumVals" : "0:开启;1:关闭",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101005,

"AttrName" : "实时监控",

"AttrType" : "操作",

"DisplayName" : "实时监控",

"EnumVals" : "0:开启;1:关闭",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101006,

"AttrName" : "对讲状态",

"AttrType" : "状态",

"DisplayName" : "对讲状态",

"EnumVals" : "0:开启;1:关闭",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101007,

"AttrName" : "开启对讲",

"AttrType" : "操作",

"DisplayName" : "开启对讲",

"EnumVals" : "0:开启;1:关闭",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : 1.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "bool",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101008,

"AttrName" : "音频类型",

"AttrType" : "配置",

"DisplayName" : "音频类型",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : 1024.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101009,

"AttrName" : "位数",

"AttrType" : "配置",

"DisplayName" : "位数",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : 1024.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101010,

"AttrName" : "采样率",

"AttrType" : "配置",

"DisplayName" : "采样率",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : 1024.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101011,

"AttrName" : "实时监控通道号",

"AttrType" : "配置",

"DisplayName" : "实时监控通道号",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 280101012,

"AttrName" : "视频回放通道号",

"AttrType" : "配置",

"DisplayName" : "视频回放通道号",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : false,

"MonitorCycle" : 5,

"OwnerCode" : 280101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290101001,

"AttrName" : "端口",

"AttrType" : "配置",

"DisplayName" : "端口",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290101000,

"ValueMax" : 65535.00,

"ValueMin" : 1.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290101003,

"AttrName" : "开机时间",

"AttrType" : "监测",

"DisplayName" : "开机时间",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "datatime",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290101004,

"AttrName" : "运行时长",

"AttrType" : "监测",

"DisplayName" : "运行时长",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "秒"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290101005,

"AttrName" : "CPU占用",

"AttrType" : "监测",

"DisplayName" : "CPU占用",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290101006,

"AttrName" : "内存使用",

"AttrType" : "监测",

"DisplayName" : "内存使用",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290101007,

"AttrName" : "硬盘使用",

"AttrType" : "监测",

"DisplayName" : "硬盘使用",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290101000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290101008,

"AttrName" : "用户连接数",

"AttrType" : "监测",

"DisplayName" : "在线用户数",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290101000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "人"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102001,

"AttrName" : "MAC地址",

"AttrType" : "配置",

"DisplayName" : "MAC地址",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102002,

"AttrName" : "网络带宽",

"AttrType" : "配置",

"DisplayName" : "网络带宽",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : 10000000.00,

"ValueMin" : 0.00,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "Kb/s"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102003,

"AttrName" : "所属AC的IP地址",

"AttrType" : "配置",

"DisplayName" : "所属AC的IP地址",

"EnumVals" : "",

"InfoPoint" : "I",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "string",

"ValueUnit" : ""

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102004,

"AttrName" : "CPU占用",

"AttrType" : "监测",

"DisplayName" : "CPU占用",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102005,

"AttrName" : "内存使用",

"AttrType" : "监测",

"DisplayName" : "内存使用",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : false,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102006,

"AttrName" : "用户连接数",

"AttrType" : "监测",

"DisplayName" : "在线用户数",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : null,

"ValueType" : "int",

"ValueUnit" : "人"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102007,

"AttrName" : "上行速率",

"AttrType" : "监测",

"DisplayName" : "上行速率",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "Kb/s"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102008,

"AttrName" : "下行速率",

"AttrType" : "监测",

"DisplayName" : "下行速率",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "Kb/s"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102009,

"AttrName" : "带宽使用率",

"AttrType" : "监测",

"DisplayName" : "带宽使用率",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : 100.00,

"ValueMin" : 0.00,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "%"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102010,

"AttrName" : "上行流量",

"AttrType" : "监测",

"DisplayName" : "上行流量",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "KB"

}, {

"AlarmHigh" : null,

"AlarmLow" : null,

"AlarmType" : -1,

"AttrCode" : 290102011,

"AttrName" : "下行流量",

"AttrType" : "监测",

"DisplayName" : "下行流量",

"EnumVals" : "",

"InfoPoint" : "O",

"IsKeypara" : true,

"IsVisible" : true,

"MonitorCycle" : 5,

"OwnerCode" : 290102000,

"ValueMax" : null,

"ValueMin" : null,

"ValuePrecision" : 1,

"ValueType" : "float",

"ValueUnit" : "KB"

} ]

**5、获取def表中定义的告警配置详情列表**

* **请求URL：**
* http://127.0.0.1:60012/WebService/GetAlarmDef
* **参数格式：**
* **请求方式：get**
* **参数：**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
|  |  |  |  |

* json返回示例：

[ {

"AlarmCause" : "",

"AlarmCode" : 990000001,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "设备故障",

"SubsysCode" : 0

}, {

"AlarmCause" : "",

"AlarmCode" : 990000002,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "防盗入侵",

"SubsysCode" : 160000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000005,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "火灾报警",

"SubsysCode" : 240000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000006,

"AlarmLevel" : 2,

"AlarmLifecycle" : 24,

"AlarmName" : "设备丢失",

"SubsysCode" : 0

}, {

"AlarmCause" : "",

"AlarmCode" : 990000007,

"AlarmLevel" : 1,

"AlarmLifecycle" : 1,

"AlarmName" : "高温告警",

"SubsysCode" : 0

}, {

"AlarmCause" : "",

"AlarmCode" : 990000008,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "过滤网告警",

"SubsysCode" : 100000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000009,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "防冻报警",

"SubsysCode" : 100000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000011,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "外部报警",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000012,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "移动侦测",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000013,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "视频遮挡",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000014,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "硬盘满",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000015,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "硬盘故障",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000016,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "视频通道异常",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000017,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "警戒线事件",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000018,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "警戒区事件",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000019,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "物品遗留事件",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000020,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "物品搬移事件",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000022,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "入侵检测",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000023,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "视频诊断",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000024,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "视频异常",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000025,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "视频丢失",

"SubsysCode" : 190000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000031,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "异常开门",

"SubsysCode" : 180000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000032,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "异常关门",

"SubsysCode" : 180000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000033,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "关门超时",

"SubsysCode" : 180000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000034,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "防拆告警",

"SubsysCode" : 180000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000035,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "胁迫开门",

"SubsysCode" : 180000000

}, {

"AlarmCause" : "",

"AlarmCode" : 990000039,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "周界仪表盖打开",

"SubsysCode" : 160000000

}, {

"AlarmCause" : "网络通信异常",

"AlarmCode" : 990000045,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "系统对象连接异常",

"SubsysCode" : 0

}, {

"AlarmCause" : "网络通信异常",

"AlarmCode" : 990000046,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "模块对象连接异常",

"SubsysCode" : 0

}, {

"AlarmCause" : "网络通信异常",

"AlarmCode" : 990000047,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "设备对象连接异常",

"SubsysCode" : 0

}, {

"AlarmCause" : null,

"AlarmCode" : 990000048,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "属性值高于阈值",

"SubsysCode" : 0

}, {

"AlarmCause" : null,

"AlarmCode" : 990000049,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "属性值低于阈值",

"SubsysCode" : 0

}, {

"AlarmCause" : null,

"AlarmCode" : 990000050,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "属性值超出范围",

"SubsysCode" : 0

}, {

"AlarmCause" : null,

"AlarmCode" : 990000053,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "进入区域",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000054,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "离开区域",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000055,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "徘徊",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000056,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "快速移动",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000057,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "人员聚集",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000058,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "场景变更",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000059,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "虚焦报警",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000060,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "物品拿取",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000061,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "物品放置拿取",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000062,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "贴条事件",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000063,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "停留事件",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000064,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "物品保全事件",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000065,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "尾随事件",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000066,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "视频损坏事件",

"SubsysCode" : 190000000

}, {

"AlarmCause" : null,

"AlarmCode" : 990000067,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "设备未配置",

"SubsysCode" : 0

}, {

"AlarmCause" : null,

"AlarmCode" : 990000068,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "通行拒绝",

"SubsysCode" : 180000000

}, {

"AlarmCause" : "灯杆上的大量设备发生告警",

"AlarmCode" : 990000069,

"AlarmLevel" : 1,

"AlarmLifecycle" : 0,

"AlarmName" : "灯杆紧急告警",

"SubsysCode" : 260000000

}, {

"AlarmCause" : "灯杆上的较多设备发生告警",

"AlarmCode" : 990000070,

"AlarmLevel" : 2,

"AlarmLifecycle" : 0,

"AlarmName" : "灯杆严重告警",

"SubsysCode" : 260000000

}, {

"AlarmCause" : "灯杆上的少量设备发生告警",

"AlarmCode" : 990000071,

"AlarmLevel" : 3,

"AlarmLifecycle" : 0,

"AlarmName" : "灯杆普通告警",

"SubsysCode" : 260000000

} ]

**6、获取def表中定义的告警类型列表**

* **请求URL：**
* http://127.0.0.1:60012/WebService/GetAlarmDefs?sysCode={sysCode}
* **参数格式：**
* **请求方式：get**
* **参数：**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
| sysCode | 否 | int | 子系统id |

* json返回示例：

[ {

"AlarmCause" : "",

"AlarmCode" : 990000001,

"AlarmLevel" : 2,

"AlarmLifecycle" : 3,

"AlarmName" : "设备故障",

"SubsysCode" : 0

}, {

"AlarmCause" : "",

"AlarmCode" : 990000006,

"AlarmLevel" : 2,

"AlarmLifecycle" : 24,

"AlarmName" : "设备丢失",

"SubsysCode" : 0

}, {

"AlarmCause" : "",

"AlarmCode" : 990000007,

"AlarmLevel" : 1,

"AlarmLifecycle" : 1,

"AlarmName" : "高温告警",

"SubsysCode" : 0

}, {

"AlarmCause" : "网络通信异常",

"AlarmCode" : 990000045,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "系统对象连接异常",

"SubsysCode" : 0

}, {

"AlarmCause" : "网络通信异常",

"AlarmCode" : 990000046,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "模块对象连接异常",

"SubsysCode" : 0

}, {

"AlarmCause" : "网络通信异常",

"AlarmCode" : 990000047,

"AlarmLevel" : 1,

"AlarmLifecycle" : 3,

"AlarmName" : "设备对象连接异常",

"SubsysCode" : 0

}, {

"AlarmCause" : null,

"AlarmCode" : 990000048,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "属性值高于阈值",

"SubsysCode" : 0

}, {

"AlarmCause" : null,

"AlarmCode" : 990000049,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "属性值低于阈值",

"SubsysCode" : 0

}, {

"AlarmCause" : null,

"AlarmCode" : 990000050,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "属性值超出范围",

"SubsysCode" : 0

}, {

"AlarmCause" : null,

"AlarmCode" : 990000067,

"AlarmLevel" : 3,

"AlarmLifecycle" : 3,

"AlarmName" : "设备未配置",

"SubsysCode" : 0

} ]

**7、获取所有告警类型的处理方式**

* **请求URL：**
* http://127.0.0.1:60012/WebService/ GetCfgTypeAlarms
* **参数格式：**
* **请求方式：get**
* **参数：**
* **Cfg表获取告警类型**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
| sysCode | 否 | int | 子系统id |

* json返回示例：

[ {

"AlarmCode" : 990000001,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 1,

"DeptId" : null,

"Id" : 1,

"Recreate" : false

}, {

"AlarmCode" : 990000002,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 2,

"Recreate" : true

}, {

"AlarmCode" : 990000005,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 5,

"Recreate" : true

}, {

"AlarmCode" : 990000006,

"AlarmLifecycle" : 24,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 6,

"Recreate" : true

}, {

"AlarmCode" : 990000007,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 7,

"Recreate" : false

}, {

"AlarmCode" : 990000008,

"AlarmLifecycle" : 3,

"AlarmWay" : 3,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 8,

"Recreate" : false

}, {

"AlarmCode" : 990000009,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 9,

"Recreate" : false

}, {

"AlarmCode" : 990000011,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 11,

"Recreate" : true

}, {

"AlarmCode" : 990000012,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 12,

"Recreate" : true

}, {

"AlarmCode" : 990000013,

"AlarmLifecycle" : 3,

"AlarmWay" : 1,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 13,

"Recreate" : true

}, {

"AlarmCode" : 990000014,

"AlarmLifecycle" : 3,

"AlarmWay" : 1,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 14,

"Recreate" : false

}, {

"AlarmCode" : 990000015,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 15,

"Recreate" : false

}, {

"AlarmCode" : 990000016,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 16,

"Recreate" : false

}, {

"AlarmCode" : 990000017,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 17,

"Recreate" : true

}, {

"AlarmCode" : 990000018,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 18,

"Recreate" : true

}, {

"AlarmCode" : 990000019,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 19,

"Recreate" : true

}, {

"AlarmCode" : 990000020,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 20,

"Recreate" : true

}, {

"AlarmCode" : 990000022,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 22,

"Recreate" : true

}, {

"AlarmCode" : 990000023,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 23,

"Recreate" : true

}, {

"AlarmCode" : 990000024,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 24,

"Recreate" : true

}, {

"AlarmCode" : 990000025,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 25,

"Recreate" : true

}, {

"AlarmCode" : 990000031,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 31,

"Recreate" : true

}, {

"AlarmCode" : 990000032,

"AlarmLifecycle" : 3,

"AlarmWay" : 1,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 32,

"Recreate" : true

}, {

"AlarmCode" : 990000033,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 33,

"Recreate" : true

}, {

"AlarmCode" : 990000034,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 34,

"Recreate" : true

}, {

"AlarmCode" : 990000035,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 35,

"Recreate" : true

}, {

"AlarmCode" : 990000039,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 39,

"Recreate" : true

}, {

"AlarmCode" : 990000045,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 24,

"DeptId" : null,

"Id" : 45,

"Recreate" : false

}, {

"AlarmCode" : 990000048,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 48,

"Recreate" : false

}, {

"AlarmCode" : 990000049,

"AlarmLifecycle" : 24,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 49,

"Recreate" : false

}, {

"AlarmCode" : 990000050,

"AlarmLifecycle" : 1,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 50,

"Recreate" : false

}, {

"AlarmCode" : 990000053,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 52,

"Recreate" : true

}, {

"AlarmCode" : 990000054,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 53,

"Recreate" : true

}, {

"AlarmCode" : 990000055,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 54,

"Recreate" : true

}, {

"AlarmCode" : 990000056,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 55,

"Recreate" : true

}, {

"AlarmCode" : 990000057,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 56,

"Recreate" : true

}, {

"AlarmCode" : 990000058,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 57,

"Recreate" : true

}, {

"AlarmCode" : 990000059,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 58,

"Recreate" : true

}, {

"AlarmCode" : 990000060,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 59,

"Recreate" : true

}, {

"AlarmCode" : 990000061,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 60,

"Recreate" : true

}, {

"AlarmCode" : 990000067,

"AlarmLifecycle" : 1,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 61,

"Recreate" : true

}, {

"AlarmCode" : 990000062,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 62,

"Recreate" : true

}, {

"AlarmCode" : 990000063,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 63,

"Recreate" : true

}, {

"AlarmCode" : 990000064,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 64,

"Recreate" : true

}, {

"AlarmCode" : 990000065,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 65,

"Recreate" : true

}, {

"AlarmCode" : 990000066,

"AlarmLifecycle" : 3,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 66,

"Recreate" : true

}, {

"AlarmCode" : 990000068,

"AlarmLifecycle" : 3,

"AlarmWay" : 0,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 68,

"Recreate" : true

}, {

"AlarmCode" : 990000046,

"AlarmLifecycle" : 1,

"AlarmWay" : 0,

"ConfirmTimeout" : 24,

"DeptId" : null,

"Id" : 70,

"Recreate" : false

}, {

"AlarmCode" : 990000047,

"AlarmLifecycle" : 1,

"AlarmWay" : 0,

"ConfirmTimeout" : 24,

"DeptId" : null,

"Id" : 71,

"Recreate" : false

}, {

"AlarmCode" : 990000069,

"AlarmLifecycle" : 0,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 72,

"Recreate" : true

}, {

"AlarmCode" : 990000070,

"AlarmLifecycle" : 0,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 73,

"Recreate" : true

}, {

"AlarmCode" : 990000071,

"AlarmLifecycle" : 0,

"AlarmWay" : null,

"ConfirmTimeout" : 0,

"DeptId" : null,

"Id" : 74,

"Recreate" : true

} ]

**8、通过设备类型获取所有的设备对象列表**

* **请求URL：**
* http://127.0.0.1:60012/WebService/GetDevices3?devType={devType}
* **参数格式：**
* **请求方式：get**
* **参数：**
* **Cfg表通过设备类型找设备**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
| devType | 是 | int | 设备类型 |

* json返回示例：

[ {

"AreaId" : 120000092,

"AreaX" : 609,

"AreaY" : 430,

"IsOnline" : true,

"Location" : null,

"Memo" : "",

"ObjectDesc" : "",

"ObjectId" : 130002019,

"ObjectIp" : "192.168.0.151",

"ObjectName" : "AP-WA748",

"ObjectType" : 290102000,

"ParentId" : 110000058,

"VendorDevid" : "",

"VendorDevname" : "WA748",

"VendorDevsn" : "D0268010011F161100527",

"VendorDevtype" : "WA748(V100R002C06B007SP5)",

"VendorName" : "敦崇"

}, {

"AreaId" : 120000092,

"AreaX" : 1091,

"AreaY" : 551,

"IsOnline" : true,

"Location" : null,

"Memo" : "",

"ObjectDesc" : "",

"ObjectId" : 130002020,

"ObjectIp" : "192.168.0.152",

"ObjectName" : "AP-测试",

"ObjectType" : 290102000,

"ParentId" : 110000058,

"VendorDevid" : "",

"VendorDevname" : "WA748",

"VendorDevsn" : "D0268010011F161100528",

"VendorDevtype" : "WA748(V100R002C06B007SP5)",

"VendorName" : "敦崇"

}, {

"AreaId" : 120000096,

"AreaX" : 432,

"AreaY" : 602,

"IsOnline" : true,

"Location" : null,

"Memo" : "",

"ObjectDesc" : "",

"ObjectId" : 130002038,

"ObjectIp" : "10.0.72.8",

"ObjectName" : "AP-B区西门",

"ObjectType" : 290102000,

"ParentId" : 110000058,

"VendorDevid" : "",

"VendorDevname" : "佛祖领社区B区西门",

"VendorDevsn" : "D0268010011F161100094",

"VendorDevtype" : "WA748(V100R002C06B007SP5)",

"VendorName" : "敦崇"

}, {

"AreaId" : 120000096,

"AreaX" : 1042,

"AreaY" : 988,

"IsOnline" : true,

"Location" : null,

"Memo" : "",

"ObjectDesc" : "",

"ObjectId" : 130002039,

"ObjectIp" : "10.0.72.23",

"ObjectName" : "AP-B区南门",

"ObjectType" : 290102000,

"ParentId" : 110000058,

"VendorDevid" : "",

"VendorDevname" : "佛祖领社区B区南门",

"VendorDevsn" : "D0268010011F161100163",

"VendorDevtype" : "WA748(V100R002C06B007SP5)",

"VendorName" : "敦崇"

}, {

"AreaId" : 120000096,

"AreaX" : 918,

"AreaY" : 83,

"IsOnline" : true,

"Location" : null,

"Memo" : "",

"ObjectDesc" : "",

"ObjectId" : 130002040,

"ObjectIp" : "10.0.72.250",

"ObjectName" : "AP-B区北门",

"ObjectType" : 290102000,

"ParentId" : 110000058,

"VendorDevid" : "",

"VendorDevname" : "佛祖领社区B区北门",

"VendorDevsn" : "D0268010011F161100186",

"VendorDevtype" : "WA748(V100R002C06B007SP5)",

"VendorName" : "敦崇"

}, {

"AreaId" : 120000096,

"AreaX" : 1517,

"AreaY" : 529,

"IsOnline" : true,

"Location" : null,

"Memo" : "",

"ObjectDesc" : "",

"ObjectId" : 130002041,

"ObjectIp" : "10.0.72.71",

"ObjectName" : "AP-B区东门",

"ObjectType" : 290102000,

"ParentId" : 110000058,

"VendorDevid" : "",

"VendorDevname" : "佛祖领社区B区东门",

"VendorDevsn" : "D0268010011F161100188",

"VendorDevtype" : "WA748(V100R002C06B007SP5)",

"VendorName" : "敦崇"

}, {

"AreaId" : 120000092,

"AreaX" : 437,

"AreaY" : 773,

"IsOnline" : true,

"Location" : null,

"Memo" : "",

"ObjectDesc" : "",

"ObjectId" : 130002044,

"ObjectIp" : "192.168.0.153",

"ObjectName" : "AP-WA612",

"ObjectType" : 290102000,

"ParentId" : 110000058,

"VendorDevid" : "",

"VendorDevname" : "WA612室外扫码设备",

"VendorDevsn" : "D0268010032F161200077",

"VendorDevtype" : "WA612",

"VendorName" : "敦崇"

} ]

**9、获取工程配置中所有的子系统对象列表**

* **请求URL：**
* <http://127.0.0.1:60012/WebService/GetSubsystems>
* **参数格式：**
* **请求方式：get**
* **参数：**
* **Cfg表获取所有子系统**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
|  |  |  |  |

* json返回示例：

[ {

"Interface" : "485",

"LinkStatus" : "0",

"LinkUrl" : "COM6",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000029,

"ObjectName" : "消防系统",

"ObjectType" : 240000000,

"Vendor" : "泛海三江",

"Version" : null

}, {

"Interface" : "SqlServer",

"LinkStatus" : "0",

"LinkUrl" : "192.168.0.200:car\_cp:sa:123456",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000031,

"ObjectName" : "停车管理",

"ObjectType" : 230000000,

"Vendor" : "毅博科技",

"Version" : null

}, {

"Interface" : "SDK",

"LinkStatus" : "0",

"LinkUrl" : "COM5:60",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000041,

"ObjectName" : "周界防盗",

"ObjectType" : 160000000,

"Vendor" : "深圳兰星",

"Version" : null

}, {

"Interface" : "SDK",

"LinkStatus" : "0",

"LinkUrl" : "10.100.20.72:9000:system:123456",

"Memo" : null,

"ObjectDesc" : "利用视频技术探测、监视设防区域并实时显示、记录现场图像的电子系统或网络",

"ObjectId" : 100000042,

"ObjectName" : "视频监控",

"ObjectType" : 190000000,

"Vendor" : "大华",

"Version" : null

}, {

"Interface" : "SDK",

"LinkStatus" : "0",

"LinkUrl" : "172.29.2.104:80:admin:admin",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000043,

"ObjectName" : "广播",

"ObjectType" : 200000000,

"Vendor" : "ITC",

"Version" : null

}, {

"Interface" : "HTTP",

"LinkStatus" : "0",

"LinkUrl" : "",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000044,

"ObjectName" : "暖通空调",

"ObjectType" : 100000000,

"Vendor" : "济南仁硕",

"Version" : null

}, {

"Interface" : "",

"LinkStatus" : "1",

"LinkUrl" : "",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000045,

"ObjectName" : "智慧路灯",

"ObjectType" : 260000000,

"Vendor" : "智慧路灯",

"Version" : null

}, {

"Interface" : "",

"LinkStatus" : "0",

"LinkUrl" : "10.100.20.72:9000:system:123456",

"Memo" : "",

"ObjectDesc" : "一键报警",

"ObjectId" : 100000047,

"ObjectName" : "一键报警",

"ObjectType" : 280000000,

"Vendor" : "大华",

"Version" : ""

}, {

"Interface" : "web serverce",

"LinkStatus" : "0",

"LinkUrl" : "https://api.xcharger.net/&1803205&E6PO0E19OX9HEX1BL2ZA6H2PTFV028EJ&10.129.76.6:9999",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000051,

"ObjectName" : "充电桩",

"ObjectType" : 270000000,

"Vendor" : "智充",

"Version" : null

}, {

"Interface" : "HTTP",

"LinkStatus" : "0",

"LinkUrl" : "120.202.24.120:9999:40001:7000",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000053,

"ObjectName" : "WIFI",

"ObjectType" : 290000000,

"Vendor" : "敦崇",

"Version" : null

}, {

"Interface" : "HTTPS",

"LinkStatus" : "0",

"LinkUrl" : "180.101.147.89:8743:dBtbXVeap04xi\_8skOK0s6U46Joa:BhagJY7j1fpMvDTHma27Lqe9bjsa:iot3rd.p12:IoM@1234",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000054,

"ObjectName" : "能耗统计",

"ObjectType" : 150000000,

"Vendor" : "电信NB-IOT",

"Version" : null

}, {

"Interface" : "OPC",

"LinkStatus" : "0",

"LinkUrl" : "",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000055,

"ObjectName" : "照明系统",

"ObjectType" : 110000000,

"Vendor" : "德易安OPC",

"Version" : null

}, {

"Interface" : "SDK",

"LinkStatus" : "0",

"LinkUrl" : "10.129.65.13:8512",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000059,

"ObjectName" : "信息发布",

"ObjectType" : 210000000,

"Vendor" : "上海仰邦",

"Version" : null

}, {

"Interface" : "Http",

"LinkStatus" : "0",

"LinkUrl" : "139c4fe135dcdcbc280418b2fa254c26&69f3d1b0150407aea259d1e800477b7f&https://interface.doordu.com/v1/&172.29.1.103&21&ibms&ibms",

"Memo" : null,

"ObjectDesc" : "",

"ObjectId" : 100000061,

"ObjectName" : "楼宇对讲",

"ObjectType" : 250000000,

"Vendor" : "伴生活",

"Version" : null

} ]

**10、获取指定子系统的模块对象列表(通过子系统找模块)**

* **请求URL：**http://127.0.0.1:60012/WebService/GetModules?subSystemId={subSystemId}
* **参数格式：**
* **请求方式：get**
* **参数：**
* **Cfg表通过子系统找模块**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
| subSystemId | 否 | int | 子系统id |

* json返回示例：

[ {

"AreaOnly" : false,

"CurrentPattern" : 0,

"IsOnline" : true,

"ObjectDesc" : null,

"ObjectId" : 110000044,

"ObjectName" : "周界防盗",

"ObjectType" : 160100000,

"ParentId" : 100000041,

"VendorName" : "深圳兰星"

} ]

**11、获取指定模块的区域对象列表(通过模块找区域)**

* **请求URL：**http://127.0.0.1:60012/WebService/GetAreas?moduleId={moduleId}
* **参数格式：**
* **请求方式：get**
* **Cfg表通过模块找区域**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
| moduleId | 否 | int | 模块id |

* json返回示例：

[ {

"MapId" : 12,

"ObjectDesc" : "",

"ObjectId" : 120000118,

"ObjectName" : "佛祖岭B区",

"ParentAreaid" : 0,

"ParentId" : 110000046,

"ParentX" : 0,

"ParentY" : 0,

"Seq" : 0

} ]

**12、获取指定模块的设备对象列表(通过模块找设备)**

* **请求URL：**http://127.0.0.1:60012/WebService/GetDevices2?moduleId={moduleId}
* **参数格式：**
* **请求方式：get**
* **参数：**
* **Cfg表通过模块找设备对象**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
| moduleId | 否 | int | 模块id |

* json返回示例：

[ {

"AreaId" : null,

"AreaX" : null,

"AreaY" : null,

"IsOnline" : true,

"Location" : "2号楼实验室",

"Memo" : "",

"ObjectDesc" : "ITC广播IP网络适配器",

"ObjectId" : 130001987,

"ObjectIp" : "10.129.65.199",

"ObjectName" : "音箱",

"ObjectType" : 200101000,

"ParentId" : 110000046,

"VendorDevid" : "6",

"VendorDevname" : "ITC播放终端",

"VendorDevsn" : "",

"VendorDevtype" : "T6700",

"VendorName" : "ITC"

}, {

"AreaId" : 120000118,

"AreaX" : 700,

"AreaY" : 368,

"IsOnline" : true,

"Location" : "2号楼实验室",

"Memo" : "",

"ObjectDesc" : "ITC广播IP网络适配器",

"ObjectId" : 130002147,

"ObjectIp" : "172.29.2.105",

"ObjectName" : "喇叭1",

"ObjectType" : 200101000,

"ParentId" : 110000046,

"VendorDevid" : "10",

"VendorDevname" : "ITC播放终端",

"VendorDevsn" : "",

"VendorDevtype" : "T67120",

"VendorName" : "ITC"

}, {

"AreaId" : 120000118,

"AreaX" : 1140,

"AreaY" : 376,

"IsOnline" : true,

"Location" : "2号楼实验室",

"Memo" : "",

"ObjectDesc" : "ITC广播IP网络适配器",

"ObjectId" : 130002148,

"ObjectIp" : "172.29.2.106",

"ObjectName" : "喇叭2",

"ObjectType" : 200101000,

"ParentId" : 110000046,

"VendorDevid" : "12",

"VendorDevname" : "ITC播放终端",

"VendorDevsn" : "",

"VendorDevtype" : "T67120",

"VendorName" : "ITC"

}, {

"AreaId" : 120000118,

"AreaX" : 965,

"AreaY" : 621,

"IsOnline" : true,

"Location" : "2号楼实验室",

"Memo" : "",

"ObjectDesc" : "ITC广播IP网络适配器",

"ObjectId" : 130002149,

"ObjectIp" : "172.29.2.108",

"ObjectName" : "喇叭4",

"ObjectType" : 200101000,

"ParentId" : 110000046,

"VendorDevid" : "13",

"VendorDevname" : "ITC播放终端",

"VendorDevsn" : "",

"VendorDevtype" : "T67120",

"VendorName" : "ITC"

} ]

### 13、获取文件资源对象列表

* **请求URL：**http://127.0.0.1:60012/WebService/GetCfgFileResource?mapId={mapId}
* **参数格式：**
* **请求方式：get**
* **参数：**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
| mapId | 否 | int | 资源id |

* json返回示例：

[ {

"resouceBody" : "data:image/png;base64,",

"resourceName" : "实验室地图-3(1).png",

"resourcePath" : "Plan/Global/",

"rid" : 1,

"updateTime" : "/Date(1513158164000+0800)/"

} ]

**14、获取指定区域的设备对象列表(通过区域找设备)**

* **请求URL：**http://127.0.0.1:60012/WebService/GetDevices1?areaId={areaId}
* **参数格式：**
* **请求方式：get**
* **参数：**
* **Cfg表通过模块找设备对象**

|  |  |  |  |
| --- | --- | --- | --- |
| **参数名** | **必选** | **类型** | **说明** |
| areaId | 否 | int | 区域id |

* json返回示例：

[ {

"AreaId" : 120000128,

"AreaX" : 1058,

"AreaY" : 554,

"IsOnline" : true,

"Location" : null,

"Memo" : null,

"ObjectDesc" : null,

"ObjectId" : 130002160,

"ObjectIp" : null,

"ObjectName" : "二号厂房2B-外",

"ObjectType" : 180103000,

"ParentId" : 110000070,

"VendorDevid" : "{ABD0F98E-702C-4E66-BAB0-AA2DD18B7274}",

"VendorDevname" : "二号厂房V1000 05#V100 二号厂房1B-外",

"VendorDevsn" : "5",

"VendorDevtype" : null,

"VendorName" : ""

} ]

### 15、获取设备表中的所有设备类型

|  |  |
| --- | --- |
| url | <http://127.0.0.1:60012/WebService/GetCfgObjDevType> |
| 请求方式 | Get |
| 参数: | 无 |
| 返回值 | [ {  "Key" : 240106000,  "Value" : "消防手动火灾报警按钮"  }, {  "Key" : 240102000,  "Value" : "消防感烟火灾探测器"  }, {  "Key" : 230103000,  "Value" : "车道"  }, {  "Key" : 230102000,  "Value" : "车位"  }, {  "Key" : 160101000,  "Value" : "周界防盗传感器"  }, {  "Key" : 190101000,  "Value" : "监控摄像机"  }, {  "Key" : 190104000,  "Value" : "硬盘录像机"  }, {  "Key" : 200101000,  "Value" : "广播终端设备"  }, {  "Key" : 100501000,  "Value" : "环境监测传感器"  }, {  "Key" : 280101000,  "Value" : "一键报警主机"  }, {  "Key" : 270101000,  "Value" : "充电桩"  }, {  "Key" : 290102000,  "Value" : "WIFI接入点"  }, {  "Key" : 150101000,  "Value" : "电表"  }, {  "Key" : 110103000,  "Value" : "无极调光回路"  }, {  "Key" : 110102000,  "Value" : "基本照明回路"  }, {  "Key" : 110101000,  "Value" : "组合照明回路"  }, {  "Key" : 210101000,  "Value" : "LED大屏幕"  }, {  "Key" : 250102000,  "Value" : "门口主机"  }, {  "Key" : 250101000,  "Value" : "围墙机"  }, {  "Key" : 180103000,  "Value" : "门禁电锁"  }, {  "Key" : 180101000,  "Value" : "门禁控制器"  }, {  "Key" : 180102000,  "Value" : "门禁读卡器"  } ] |

### 16、获取子系统在线信息

|  |  |
| --- | --- |
| url | <http://127.0.0.1:60012/WebService/GetSubSystemOnlineInfo> |
| 请求方式 | Get |
| 参数: | 无 |
| 返回值 | [ {  "Key" : 100000029,  "Value" : 0  }, {  "Key" : 100000031,  "Value" : 0  }, {  "Key" : 100000041,  "Value" : 0  }, {  "Key" : 100000042,  "Value" : 0  }, {  "Key" : 100000043,  "Value" : 0  }, {  "Key" : 100000044,  "Value" : 0  }, {  "Key" : 100000047,  "Value" : 0  }, {  "Key" : 100000051,  "Value" : 0  }, {  "Key" : 100000053,  "Value" : 0  }, {  "Key" : 100000054,  "Value" : 0  }, {  "Key" : 100000055,  "Value" : 0  }, {  "Key" : 100000059,  "Value" : 0  }, {  "Key" : 100000061,  "Value" : 0  }, {  "Key" : 100000062,  "Value" : 0  } ] |

### 17、获取广播音乐文件

|  |  |
| --- | --- |
| url | [http://127.0.0.1:60012/WebService/](http://127.0.0.1:60012/WebService/GetSubSystemOnlineInfo)GetBroadcastFileList |
| 请求方式 | Get |
| 参数: | 无 |
| 返回值 | [ {  "Fid" : 1,  "FileName" : "IntrusionAlarm",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "193",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 2,  "FileName" : "ring",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "194",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 3,  "FileName" : "xring",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "195",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 4,  "FileName" : "第九套大众广播体操",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "201",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 5,  "FileName" : "起床号",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "202",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 6,  "FileName" : "整队做课间操口令",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "203",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 7,  "FileName" : "陈慧琳 - 记事本",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "204",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 8,  "FileName" : "邓紫棋 - 喜欢你",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "205",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 9,  "FileName" : "范玮琪 - 最初的梦想",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "206",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 10,  "FileName" : "方力申、邓丽欣 - 好心好报",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "207",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 11,  "FileName" : "龚玥 - 大悲咒 - 佛歌 高质量",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "208",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 12,  "FileName" : "胡杏儿 - 小幸运 (Live)",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "209",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 13,  "FileName" : "经典英文老歌",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "210",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 14,  "FileName" : "冷漠 - 伤心城市",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "211",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 15,  "FileName" : "李克勤 - 一生不变",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "212",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 16,  "FileName" : "刘德华 - 我恨我痴心",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "213",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 17,  "FileName" : "孙露 - 一定要爱你",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "214",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 18,  "FileName" : "王菲 - 传奇",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "215",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 19,  "FileName" : "薛之谦 - 演员",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "216",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 20,  "FileName" : "张学友 - 一路上有你",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "223",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 21,  "FileName" : "张学友 - 只想一生跟你走",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "224",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 22,  "FileName" : "周传雄 - 男人·海洋",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "225",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 23,  "FileName" : "周传雄 - 我的心太乱",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "226",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 24,  "FileName" : "周亮 - 莫生气",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "227",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 25,  "FileName" : "浏阳河 - 古筝独奏 送 别 古筝",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "229",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 26,  "FileName" : "一剪梅",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "230",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 27,  "FileName" : "月光下的凤尾竹胡芦丝",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "231",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 28,  "FileName" : "CBR\_张学友 - 爱很简单",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "196",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 29,  "FileName" : "nana - lonely",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "197",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 30,  "FileName" : "蔡健雅 - 当我想你的时候",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "198",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 31,  "FileName" : "纯音乐",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "199",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 32,  "FileName" : "梁祝钢琴曲",  "FileType" : 1,  "Flag" : null,  "RemoteFid" : "200",  "RemoteType" : 0,  "VendorName" : "ITC"  }, {  "Fid" : 38,  "FileName" : "光的方向\_测试",  "FileType" : 1,  "Flag" : 0,  "RemoteFid" : "0",  "RemoteType" : 0,  "VendorName" : "ITC"  } ] |

### 18、获取设备集合的所有属性列表

|  |  |
| --- | --- |
| url | <http://127.0.0.1:60012/WebService/GetAttrsByObjList?objIdList=130001987,130001988,130002048> |
| 请求方式 | Get |
| 参数: | 无 |
| 返回值 | [{"AlarmHigh":null,"AlarmLow":null,"AlarmType":0,"ObjectId":140001082,"ObjectName":"监听音箱音量","ObjectType":200101001,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"22","VendorAttrId":"3"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001083,"ObjectName":"监听音箱运行状态","ObjectType":200101002,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"4"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001084,"ObjectName":"监听音箱播放节目","ObjectType":200101003,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"5"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001085,"ObjectName":"监听音箱播放文件","ObjectType":200101004,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"6"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001086,"ObjectName":"监听音箱播放任务","ObjectType":200101005,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"7"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001087,"ObjectName":"摄像机工作状态","ObjectType":190101001,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1528268400000+0800)\/","ValueStr":"0","VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001088,"ObjectName":"摄像机告警状态","ObjectType":190101002,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":"0","VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001089,"ObjectName":"摄像机型号","ObjectType":190101003,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":null,"VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001090,"ObjectName":"摄像机端口号","ObjectType":190101004,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":null,"VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001091,"ObjectName":"摄像机用户名","ObjectType":190101005,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":null,"VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001092,"ObjectName":"摄像机密码","ObjectType":190101006,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":null,"VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001093,"ObjectName":"摄像机序列号","ObjectType":190101007,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":null,"VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001094,"ObjectName":"摄像机联系人","ObjectType":190101008,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":null,"VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001095,"ObjectName":"摄像机联系人号码","ObjectType":190101009,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":null,"VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001096,"ObjectName":"摄像机权限","ObjectType":190101010,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":null,"VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001097,"ObjectName":"实时监控","ObjectType":190101011,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1528268400000+0800)\/","ValueStr":"0","VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001098,"ObjectName":"视频轮巡","ObjectType":190101012,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1528268400000+0800)\/","ValueStr":"0","VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001099,"ObjectName":"点间巡航","ObjectType":190101013,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1528268400000+0800)\/","ValueStr":"0","VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001100,"ObjectName":"摄像机类型","ObjectType":190101014,"OwnerObjectid":130001988,"UpdateTime":"\/Date(1523116800000+0800)\/","ValueStr":"3","VendorAttrId":""},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":0,"ObjectId":140001371,"ObjectName":"灯杆5\_照明电表\_电表读数","ObjectType":150101001,"OwnerObjectid":130002048,"UpdateTime":"\/Date(1536113400000+0800)\/","ValueStr":"8.37","VendorAttrId":"powerLevel3"}] |

### 19、获取设备对象的属性列表

|  |  |
| --- | --- |
| url | <http://127.0.0.1:60012/WebService/GetAttrs?oId=130001987> |
| 请求方式 | Get |
| 参数: | 无 |
| 返回值 | [{"AlarmHigh":null,"AlarmLow":null,"AlarmType":0,"ObjectId":140001082,"ObjectName":"监听音箱音量","ObjectType":200101001,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"22","VendorAttrId":"3"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001083,"ObjectName":"监听音箱运行状态","ObjectType":200101002,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"4"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001084,"ObjectName":"监听音箱播放节目","ObjectType":200101003,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"5"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001085,"ObjectName":"监听音箱播放文件","ObjectType":200101004,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"6"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001086,"ObjectName":"监听音箱播放任务","ObjectType":200101005,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"7"}] |

### 20、获取指定对象的属性列表(子系统id、模块id、区域id、设备id)

|  |  |
| --- | --- |
| url | <http://127.0.0.1:60012/WebService/GetAttrsByObjId?objId=130001987> |
| 请求方式 | Get |
| 参数: | 无 |
| 返回值 | [{"AlarmHigh":null,"AlarmLow":null,"AlarmType":0,"ObjectId":140001082,"ObjectName":"监听音箱音量","ObjectType":200101001,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"22","VendorAttrId":"3"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001083,"ObjectName":"监听音箱运行状态","ObjectType":200101002,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"4"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001084,"ObjectName":"监听音箱播放节目","ObjectType":200101003,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"5"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001085,"ObjectName":"监听音箱播放文件","ObjectType":200101004,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"6"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001086,"ObjectName":"监听音箱播放任务","ObjectType":200101005,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"7"}] |

### 21、通过系统码获取子系统详细信息

|  |  |
| --- | --- |
| url | http://127.0.0.1:60012/WebService/GetSystemDetailInfo?systemCode=200000000 |
| 请求方式 | Get |
| 参数: | 无 |
| 返回值 | {"cfgAreaList":[{"MapId":12,"ObjectDesc":"","ObjectId":120000118,"ObjectName":"佛祖岭B区","ParentAreaid":0,"ParentId":110000046,"ParentX":0,"ParentY":0,"Seq":0}],"cfgModuleList":[{"AreaOnly":false,"CurrentPattern":0,"IsOnline":true,"ObjectDesc":"广州ITC公共广播系统模块","ObjectId":110000046,"ObjectName":"广播","ObjectType":200100000,"ParentId":100000043,"VendorName":"ITC"}],"cfgObjectAttrList":[{"AlarmHigh":null,"AlarmLow":null,"AlarmType":0,"ObjectId":140001082,"ObjectName":"监听音箱音量","ObjectType":200101001,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"22","VendorAttrId":"3"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001083,"ObjectName":"监听音箱运行状态","ObjectType":200101002,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"4"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001084,"ObjectName":"监听音箱播放节目","ObjectType":200101003,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"5"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001085,"ObjectName":"监听音箱播放文件","ObjectType":200101004,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"6"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001086,"ObjectName":"监听音箱播放任务","ObjectType":200101005,"OwnerObjectid":130001987,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"7"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":0,"ObjectId":140001621,"ObjectName":"喇叭1音量","ObjectType":200101001,"OwnerObjectid":130002147,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"6","VendorAttrId":"3"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001622,"ObjectName":"喇叭1运行状态","ObjectType":200101002,"OwnerObjectid":130002147,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"1","VendorAttrId":"4"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001623,"ObjectName":"喇叭1播放节目","ObjectType":200101003,"OwnerObjectid":130002147,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"5"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001624,"ObjectName":"喇叭1播放文件","ObjectType":200101004,"OwnerObjectid":130002147,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"6"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001625,"ObjectName":"喇叭1播放任务","ObjectType":200101005,"OwnerObjectid":130002147,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"7"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":0,"ObjectId":140001626,"ObjectName":"喇叭2音量","ObjectType":200101001,"OwnerObjectid":130002148,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"6","VendorAttrId":"8"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001627,"ObjectName":"喇叭2运行状态","ObjectType":200101002,"OwnerObjectid":130002148,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"1","VendorAttrId":"9"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001628,"ObjectName":"喇叭2播放节目","ObjectType":200101003,"OwnerObjectid":130002148,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"10"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001629,"ObjectName":"喇叭2播放文件","ObjectType":200101004,"OwnerObjectid":130002148,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"11"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001630,"ObjectName":"喇叭2播放任务","ObjectType":200101005,"OwnerObjectid":130002148,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"12"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":0,"ObjectId":140001631,"ObjectName":"喇叭4音量","ObjectType":200101001,"OwnerObjectid":130002149,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"4","VendorAttrId":"13"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001632,"ObjectName":"喇叭4运行状态","ObjectType":200101002,"OwnerObjectid":130002149,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"1","VendorAttrId":"14"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001633,"ObjectName":"喇叭4播放节目","ObjectType":200101003,"OwnerObjectid":130002149,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"15"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001634,"ObjectName":"喇叭4播放文件","ObjectType":200101004,"OwnerObjectid":130002149,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"","VendorAttrId":"16"},{"AlarmHigh":null,"AlarmLow":null,"AlarmType":-1,"ObjectId":140001635,"ObjectName":"喇叭4播放任务","ObjectType":200101005,"OwnerObjectid":130002149,"UpdateTime":"\/Date(1538204113000+0800)\/","ValueStr":"0","VendorAttrId":"17"}],"cfgObjectList":[{"AreaId":120000118,"AreaX":null,"AreaY":null,"IsOnline":true,"Location":"2号楼实验室","Memo":"","ObjectDesc":"ITC广播IP网络适配器","ObjectId":130001987,"ObjectIp":"10.129.65.199","ObjectName":"音箱","ObjectType":200101000,"ParentId":110000046,"VendorDevid":"6","VendorDevname":"ITC播放终端","VendorDevsn":"","VendorDevtype":"T6700","VendorName":"ITC"},{"AreaId":120000118,"AreaX":700,"AreaY":368,"IsOnline":true,"Location":"2号楼实验室","Memo":"","ObjectDesc":"ITC广播IP网络适配器","ObjectId":130002147,"ObjectIp":"172.29.2.105","ObjectName":"喇叭1","ObjectType":200101000,"ParentId":110000046,"VendorDevid":"10","VendorDevname":"ITC播放终端","VendorDevsn":"","VendorDevtype":"T67120","VendorName":"ITC"},{"AreaId":120000118,"AreaX":1140,"AreaY":376,"IsOnline":true,"Location":"2号楼实验室","Memo":"","ObjectDesc":"ITC广播IP网络适配器","ObjectId":130002148,"ObjectIp":"172.29.2.106","ObjectName":"喇叭2","ObjectType":200101000,"ParentId":110000046,"VendorDevid":"12","VendorDevname":"ITC播放终端","VendorDevsn":"","VendorDevtype":"T67120","VendorName":"ITC"},{"AreaId":120000118,"AreaX":965,"AreaY":621,"IsOnline":true,"Location":"2号楼实验室","Memo":"","ObjectDesc":"ITC广播IP网络适配器","ObjectId":130002149,"ObjectIp":"172.29.2.108","ObjectName":"喇叭4","ObjectType":200101000,"ParentId":110000046,"VendorDevid":"13","VendorDevname":"ITC播放终端","VendorDevsn":"","VendorDevtype":"T67120","VendorName":"ITC"}],"cfgSystem":{"Interface":"SDK","LinkStatus":"0","LinkUrl":"172.29.2.104:80:admin:admin","Memo":null,"ObjectDesc":"","ObjectId":100000043,"ObjectName":"广播","ObjectType":200000000,"Vendor":"ITC","Version":null}} |